<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ALPHANUMERIC">
</package>
<package name="LCD-16X2">
</package>
<package name="LCD-16X2_NOSILK">
</package>
<package name="LCD-16X2_NOHOLES">
</package>
<package name="LCD-8X2">
<description>&lt;h3&gt;8x2 Character LCD w/ Backlight&lt;/h3&gt;
Outer Dimensions: 40.0 x 35.4mm&lt;br&gt;
Viewing Area: 26.4 x 13.9mm&lt;br&gt;
Character Size: 2.95 x 4.75mm&lt;br&gt;
&lt;br&gt;
For Reference, see Amotec Display part ADM0802A (http://amotec-display.com/pdf/ADM0802A.pdf).
&lt;br&gt;
&lt;br&gt;
&lt;B&gt;***Footprint Unproven***&lt;/b&gt;</description>
</package>
<package name="LCD-8X2-KIT">
<description>&lt;h3&gt;LCD-8X2-KIT&lt;/h3&gt;
8x2 LCD&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="LCD-G12864">
</package>
<package name="1X20">
</package>
<package name="LCD_BACKLIGHT_PADS">
</package>
<package name="LCD_CFAX">
</package>
<package name="NOKIA6100_LCD">
</package>
<package name="SCREENKEY-TFT128">
</package>
<package name="7-SEGMENT-4DIGIT">
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN">
<description>This is a package for the 4-digit 7-segment RED LED from Young Sun.</description>
</package>
<package name="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
</package>
<package name="7-SEGMENT-DISPLAY">
</package>
<package name="7-SEGMENT-1&quot;PTH">
<description>7 Segment display Storefront SKU#: COM-08546</description>
</package>
<package name="7-SEGMENT-4DIGIT-COUNTER">
</package>
</packages>
<symbols>
<symbol name="ALPHANUMERIC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="H"/>
<pin name="J"/>
<pin name="K"/>
<pin name="L"/>
<pin name="M"/>
<pin name="N"/>
<pin name="NC@1"/>
<pin name="NC@13"/>
<pin name="VCC@6"/>
<pin name="VCC@18"/>
</symbol>
<symbol name="LCD-16X2">
<pin name="A" direction="pwr"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="E" direction="in"/>
<pin name="K" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VO"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LCD-G12864">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VO"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="D/I" direction="in"/>
<pin name="E" direction="in"/>
<pin name="VEE"/>
<pin name="A" direction="pwr"/>
<pin name="K" direction="pwr"/>
</symbol>
<symbol name="LCD_BACKLIGHT_PADS">
<pin name="A"/>
<pin name="K"/>
</symbol>
<symbol name="LCD_CFAX">
<pin name="VCC"/>
<pin name="RESET"/>
<pin name="GND"/>
<pin name="CS1B"/>
<pin name="CS2"/>
<pin name="RS"/>
<pin name="RW"/>
<pin name="ERD"/>
<pin name="MI"/>
<pin name="P/S"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
</symbol>
<symbol name="NOKIA6100_LCD">
<pin name="VDISPLAY"/>
<pin name="VDIGITAL"/>
<pin name="SCK"/>
<pin name="DIO"/>
<pin name="CS"/>
<pin name="GND"/>
<pin name="LEDGND"/>
<pin name="RESET"/>
<pin name="VLED"/>
</symbol>
<symbol name="SCREENKEY-TFT128">
</symbol>
<symbol name="7-SEGMENT-4DIGIT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="11"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-YOUNGSUN">
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="COL-A"/>
<pin name="APOS-A"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="COL-C"/>
<pin name="APOS-C"/>
<pin name="DIG1"/>
</symbol>
<symbol name="7-SEGMENT-DISPLAY">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="DP"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="7-SEGMENT-1&quot;">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-COUNTER">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ALPHANUMERIC" prefix="U">
<description>&lt;b&gt;Alphanumeric LED Display&lt;/b&gt; Common anode. Multiple LEDs on some segments. Multiple LED colors available. Works great with A6282 driver IC. Decimal points are unfornately not connected. SKU: COM-09933.</description>
<gates>
<gate name="G$1" symbol="ALPHANUMERIC"/>
</gates>
<devices>
<device name="PTH" package="ALPHANUMERIC">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="B" pad="21"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="14"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="F" pad="4"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="19"/>
<connect gate="G$1" pin="H" pad="3"/>
<connect gate="G$1" pin="J" pad="24"/>
<connect gate="G$1" pin="K" pad="23"/>
<connect gate="G$1" pin="L" pad="15"/>
<connect gate="G$1" pin="M" pad="12"/>
<connect gate="G$1" pin="N" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@13" pad="13"/>
<connect gate="G$1" pin="VCC@18" pad="18"/>
<connect gate="G$1" pin="VCC@6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-16X2" prefix="U">
<description>Standard text-only 16x2 parallel input LCD</description>
<gates>
<gate name="G$1" symbol="LCD-16X2"/>
</gates>
<devices>
<device name="SILK" package="LCD-16X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="LCD-16X2_NOSILK">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="LCD-16X2_NOHOLES">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X2" package="LCD-8X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X2-KIT" package="LCD-8X2-KIT">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-G12864">
<description>&lt;b&gt;Graphical LCD 128x64&lt;/b&gt; 
Footprint is not yet proven. Double check it. Spark Fun Electronics SKU : LCD-00710</description>
<gates>
<gate name="G$1" symbol="LCD-G12864"/>
</gates>
<devices>
<device name="FULL" package="LCD-G12864">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BARE" package="1X20">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_BACKLIGHT_PADS">
<gates>
<gate name="G$1" symbol="LCD_BACKLIGHT_PADS"/>
</gates>
<devices>
<device name="" package="LCD_BACKLIGHT_PADS">
<connects>
<connect gate="G$1" pin="A" pad="P$1"/>
<connect gate="G$1" pin="K" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_CFAX">
<description>Graphic LCD module (LCD-00463) DISCONTINUED</description>
<gates>
<gate name="LCD" symbol="LCD_CFAX"/>
</gates>
<devices>
<device name="" package="LCD_CFAX">
<connects>
<connect gate="LCD" pin="CS1B" pad="P$3"/>
<connect gate="LCD" pin="CS2" pad="P$4"/>
<connect gate="LCD" pin="D0" pad="P$9"/>
<connect gate="LCD" pin="D1" pad="P$10"/>
<connect gate="LCD" pin="D2" pad="P$11"/>
<connect gate="LCD" pin="D3" pad="P$12"/>
<connect gate="LCD" pin="D4" pad="P$13"/>
<connect gate="LCD" pin="D5" pad="P$14"/>
<connect gate="LCD" pin="D6" pad="P$15"/>
<connect gate="LCD" pin="D7" pad="P$16"/>
<connect gate="LCD" pin="ERD" pad="P$8"/>
<connect gate="LCD" pin="GND" pad="P$2"/>
<connect gate="LCD" pin="MI" pad="P$17"/>
<connect gate="LCD" pin="P/S" pad="P$18"/>
<connect gate="LCD" pin="RESET" pad="P$5"/>
<connect gate="LCD" pin="RS" pad="P$6"/>
<connect gate="LCD" pin="RW" pad="P$7"/>
<connect gate="LCD" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NOKIA6100_LCD">
<description>&lt;b&gt;Nokia 6100 Color LCD&lt;/b&gt;
Schematic element and footprint production proven but could use some touching up. Spark Fun Electronics SKU : LCD-00569. Mating SMD connector : LCD-00570</description>
<gates>
<gate name="G$1" symbol="NOKIA6100_LCD"/>
</gates>
<devices>
<device name="" package="NOKIA6100_LCD">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DIO" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LEDGND" pad="9"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VDIGITAL" pad="1"/>
<connect gate="G$1" pin="VDISPLAY" pad="6"/>
<connect gate="G$1" pin="VLED" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREENKEY-TFT128">
<description>Mechanical footprint of the ScreenKey (COM-09366)&lt;br&gt;
NO ELECTRICAL CONNECTIONS.</description>
<gates>
<gate name="G$1" symbol="SCREENKEY-TFT128"/>
</gates>
<devices>
<device name="DEMENSIONANDHOLES" package="SCREENKEY-TFT128">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT">
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-4DIGIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOR_POGOBED_ONLY" package="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT-YOUNGSUN" prefix="LED">
<description>This is a part for the 4-Digit 7-segment LEDs from Young Sun.  Different from the Digikey LEDs, all 16 pins are used.
The LONGPADS Variant is used for a test jig, but you may like it because there is more pad to solder to. If you are concerned about routing space, the standard works just fine though.</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-YOUNGSUN"/>
</gates>
<devices>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-DISPLAY">
<gates>
<gate name="G$1" symbol="7-SEGMENT-DISPLAY"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-DISPLAY">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-DISPLAY-1&quot;-RED">
<description>7-Segment Display 1" Red (COM-08546)</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-1&quot;"/>
</gates>
<devices>
<device name="" package="7-SEGMENT-1&quot;PTH">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT-COUNTER">
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-COUNTER"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-4DIGIT-COUNTER">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
