<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Linear Technology Devices&lt;/b&gt;&lt;p&gt;
http://www.linear-tech.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="Q5-DD">
<description>&lt;b&gt;Q5-DD&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="TO220-5">
<description>&lt;b&gt;TO220-5&lt;/b&gt;</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;MSOP8&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SSOP36">
<description>&lt;b&gt;G Package 36-Lead Plastic SSOP (0.209)&lt;/b&gt;&lt;p&gt;
LTC DWG # 05-08-1640&lt;br&gt;
Source: www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1143,C1083,P1964,D1133</description>
</package>
<package name="DFN10-3X3">
<description>&lt;b&gt;DD Package 10-Lead Plastic DFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
(Reference LTC DWG # 05-08-1669)&lt;br&gt;
Source: http://www.linear.com .. 4062fa.pdf</description>
</package>
<package name="SO28SW">
<description>&lt;B&gt;28-Lead Plastic Small Outline Isolation Barrier&lt;/b&gt; (Wide .300 Inch)&lt;p&gt;
Reference LTC DWG # 05-08-1690&lt;br&gt;
Source: www.linear.com</description>
</package>
<package name="DFN6-2X3">
<description>&lt;b&gt;DCB Package 6-Lead Plastic DFN (2mm × 3mm)&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1032,C1063,P26952,D16357</description>
</package>
<package name="DFN14-4X3DE">
<description>&lt;b&gt;14-LEAD (4mm x 2mm) PALSTIC DFN&lt;/b&gt; DE14MA PACKAGE&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1032,C1064,P38040,D25144</description>
</package>
<package name="QFN64-9X9">
<description>&lt;b&lt;WP Package&lt;/b&gt; 64-Lead QFN Multipad (9mm × 9mm)&lt;p&gt;
Source: http://www.linear.com ..</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead Platic MSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. LT1996</description>
</package>
<package name="DFN14-4X3">
<description>&lt;b&gt;14-Lead Plastic DFN&lt;/b&gt; (4mm × 3mm)&lt;p&gt;
(Reference LTC DWG # 05-08-1708 Rev B)&lt;br&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1155,C1001,C1152,P36532,D19318</description>
</package>
<package name="LGA50">
<description>&lt;b&gt;LGA Package&lt;/b&gt; 50-Lead (11.25mm × 9.00mm × 2.82mm)&lt;p&gt;
(Reference LTC DWG # 05-08-1804 Rev B)&lt;br&gt;
Source: http://www.linear.com .. 8023fc.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;16-Lead Plastic TSSOP (4.4mm)&lt;/b&gt;&lt;p&gt;
http://cds.linear.com/docs/Datasheet/1963fc.pdf</description>
</package>
<package name="TSSOP16EXP">
<description>&lt;b&gt;16-Lead Plastic TSSOP (4.4mm) EXPOSED PAD&lt;/b&gt;&lt;p&gt;
http://cds.linear.com/docs/Datasheet/1963fc.pdf</description>
</package>
<package name="DFN12">
<description>&lt;b&gt;DE/UE Package 12-Lead Plastic DFN (4mm × 3mm)&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/1763ff.pdf</description>
</package>
<package name="S8">
<description>&lt;b&gt;8-Lead Plastic Small Outline&lt;/b&gt; Narrow .150 Inch&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="DFN8-3X3">
<description>&lt;b&gt;DD Package 8-Lead Plastic DFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="TSOT23-6">
<description>&lt;b&gt;S6 Package 6-Lead Plastic TSOT-23&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;GN Package 16-Lead Plastic SSOP (Narrow .150 Inch)&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="QFN24-4X4">
<description>&lt;b&gt;UF Package 24-Lead (4mm × 4mm) Plastic QFN&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/5598f.pdf</description>
</package>
<package name="DFN8-2X3">
</package>
</packages>
<symbols>
<symbol name="LT1129">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="LT1129-3">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1016">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="LA_EN" direction="in"/>
<pin name="!OUT" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LTC1658">
<pin name="DOUT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="!CSLD" direction="in"/>
</symbol>
<symbol name="LTC1709-7">
<pin name="FCB" direction="pas"/>
<pin name="RUN/SS" direction="in"/>
<pin name="ITH" direction="out"/>
<pin name="SGND" direction="pwr"/>
<pin name="PGOOD" direction="out"/>
<pin name="VID0" direction="in"/>
<pin name="VID1" direction="in"/>
<pin name="VID2" direction="in"/>
<pin name="VID3" direction="in"/>
<pin name="VID4" direction="in"/>
<pin name="EAIN" direction="in"/>
<pin name="ATTENOUT" direction="out"/>
<pin name="ATTENIN" direction="in"/>
<pin name="VDIFFOUT" direction="out"/>
<pin name="VOS-" direction="in"/>
<pin name="VOS+" direction="in"/>
<pin name="SENSE2-" direction="in"/>
<pin name="SENSE2+" direction="in"/>
<pin name="INTVCC" direction="in"/>
<pin name="BG2" direction="out"/>
<pin name="SW2" direction="pas"/>
<pin name="BOOST2" direction="pas"/>
<pin name="TG2" direction="out"/>
<pin name="SENSE1-" direction="in"/>
<pin name="SENSE1+" direction="in"/>
<pin name="PGND" direction="in"/>
<pin name="BG1" direction="out"/>
<pin name="SW1" direction="pas"/>
<pin name="BOOST1" direction="pas"/>
<pin name="TG1" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="PLLIN" direction="in"/>
<pin name="PLLFLTR" direction="pas"/>
<pin name="EXTVCC" direction="in"/>
<pin name="VBIAS" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="LTC4062">
<pin name="IN+" direction="in"/>
<pin name="OUT" direction="oc"/>
<pin name="!CHRG" direction="oc"/>
<pin name="!C/5" direction="in"/>
<pin name="!EN" direction="in"/>
<pin name="TIMER" direction="pas"/>
<pin name="IDET" direction="pas"/>
<pin name="PROG" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="BAT" direction="pas"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LTC1288">
<pin name="DOUT" direction="out"/>
<pin name="!CS!/SHDN" direction="out"/>
<pin name="+IN/C0" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="-IN/C1" direction="in"/>
</symbol>
<symbol name="LTC2602">
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="!CS/LD" direction="in"/>
</symbol>
<symbol name="LTC1535">
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RO" direction="out"/>
<pin name="!RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="ST1" direction="in"/>
<pin name="ST2" direction="in"/>
<pin name="GND2" direction="in"/>
<pin name="VCC2" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="RO2" direction="out"/>
<pin name="Y" direction="hiz"/>
<pin name="Z" direction="hiz"/>
<pin name="!SLO" direction="in"/>
</symbol>
<symbol name="LTC485">
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RO" direction="out"/>
<pin name="!RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="LT1963">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LT1963ET">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1021">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LTC3549">
<pin name="IN" direction="in"/>
<pin name="SW" direction="out"/>
<pin name="RUN" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="LT3681">
<pin name="PG" direction="oc"/>
<pin name="BIAS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VC" direction="out"/>
<pin name="RT" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="DA" direction="pas"/>
<pin name="DC" direction="pas"/>
<pin name="BD" direction="in"/>
<pin name="BOOST" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="RUN/SS" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="DC@1" direction="pas"/>
</symbol>
<symbol name="LT1168">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="RG@2" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="in"/>
</symbol>
<symbol name="LT1236">
<pin name="VIN" direction="in"/>
<pin name="OUT" direction="in"/>
<pin name="TRIM" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1257">
<pin name="DOUT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="!LOAD" direction="in"/>
</symbol>
<symbol name="LTC3610">
<pin name="PGND@1" direction="pwr"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="PGND@3" direction="pwr"/>
<pin name="PGND@4" direction="pwr"/>
<pin name="PGND@5" direction="pwr"/>
<pin name="PGND@6" direction="pwr"/>
<pin name="PGND@7" direction="pwr"/>
<pin name="PGND@8" direction="pwr"/>
<pin name="PGND@9" direction="pwr"/>
<pin name="PGND@10" direction="pwr"/>
<pin name="PGND@11" direction="pwr"/>
<pin name="PGND@12" direction="pwr"/>
<pin name="PVIN@1" direction="pwr"/>
<pin name="PVIN@2" direction="pwr"/>
<pin name="PVIN@3" direction="pwr"/>
<pin name="PVIN@4" direction="pwr"/>
<pin name="PVIN@5" direction="pwr"/>
<pin name="PVIN@6" direction="pwr"/>
<pin name="PVIN@7" direction="pwr"/>
<pin name="PVIN@8" direction="pwr"/>
<pin name="PVIN@9" direction="pwr"/>
<pin name="PVIN@10" direction="pwr"/>
<pin name="PVIN@11" direction="pwr"/>
<pin name="PVIN@12" direction="pwr"/>
<pin name="PVIN@13" direction="pwr"/>
<pin name="PVIN@14" direction="pwr"/>
<pin name="SGND@1" direction="pwr"/>
<pin name="SGND@2" direction="pwr"/>
<pin name="SGND@3" direction="pwr"/>
<pin name="SGND@4" direction="pwr"/>
<pin name="SGND@5" direction="pwr"/>
<pin name="SGND@6" direction="pwr"/>
<pin name="SGND@7" direction="pwr"/>
<pin name="SGND@8" direction="pwr"/>
<pin name="SGND@9" direction="pwr"/>
<pin name="SGND@10" direction="pwr"/>
<pin name="SGND@11" direction="pwr"/>
<pin name="SGND@12" direction="pwr"/>
<pin name="INTVCC@1" direction="pwr"/>
<pin name="INTVCC@2" direction="pwr"/>
<pin name="SW@1" direction="in"/>
<pin name="SW@2" direction="in"/>
<pin name="SW@3" direction="in"/>
<pin name="SW@4" direction="in"/>
<pin name="SW@5" direction="in"/>
<pin name="SW@6" direction="in"/>
<pin name="SW@7" direction="in"/>
<pin name="SW@8" direction="in"/>
<pin name="SW@9" direction="in"/>
<pin name="SW@10" direction="in"/>
<pin name="SVIN@1" direction="in"/>
<pin name="SVIN@2" direction="in"/>
<pin name="EXTVCC" direction="in"/>
<pin name="VFB" direction="pas"/>
<pin name="ION" direction="in"/>
<pin name="FCB" direction="pas"/>
<pin name="ITH" direction="pas"/>
<pin name="VRNG" direction="pas"/>
<pin name="PGOOD" direction="oc"/>
<pin name="VON" direction="in"/>
<pin name="RUN/SS" direction="pas"/>
<pin name="BOOST" direction="pas"/>
<pin name="PVIN@15" direction="pwr"/>
<pin name="SW@11" direction="in"/>
<pin name="PGND@13" direction="pwr"/>
<pin name="SGND@13" direction="pwr"/>
</symbol>
<symbol name="LTC3610-P">
<pin name="SGND@1" direction="pwr"/>
<pin name="SVIN@6" direction="in"/>
<pin name="INTVCC@1" direction="pwr"/>
<pin name="SVIN@1" direction="in"/>
<pin name="SVIN@2" direction="in"/>
<pin name="INTVCC@2" direction="pwr"/>
<pin name="INTVCC@3" direction="pwr"/>
<pin name="INTVCC@4" direction="pwr"/>
<pin name="SVIN@3" direction="in"/>
<pin name="SVIN@4" direction="in"/>
<pin name="SVIN@5" direction="in"/>
<pin name="INTVCC@5" direction="pwr"/>
</symbol>
<symbol name="LT1996">
<pin name="P81" direction="in"/>
<pin name="M81" direction="in"/>
<pin name="M27" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="P27" direction="in"/>
<pin name="P9" direction="in"/>
<pin name="M9" direction="in"/>
</symbol>
<symbol name="LTC2486">
<pin name="FO" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="COM" direction="pwr"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="EXP" direction="in"/>
</symbol>
<symbol name="LTC2482">
<pin name="FO" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="EXP" direction="in"/>
<pin name="GND@*" direction="pwr"/>
</symbol>
<symbol name="LTM8023">
<pin name="VIN" direction="pwr"/>
<pin name="SHARE" direction="in"/>
<pin name="RUN/SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="BIAS" direction="pas"/>
<pin name="PGOOD" direction="oc"/>
<pin name="ADJ" direction="pas"/>
<pin name="RT" direction="pas"/>
<pin name="AUX" direction="out"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="LTM8023-P">
<pin name="VIN@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VOUT@1" direction="pwr"/>
<pin name="VIN@2" direction="pwr"/>
<pin name="VIN@3" direction="pwr"/>
<pin name="VIN@4" direction="pwr"/>
<pin name="VIN@5" direction="pwr"/>
<pin name="VOUT@2" direction="pwr"/>
<pin name="VOUT@3" direction="pwr"/>
<pin name="VOUT@4" direction="pwr"/>
<pin name="VOUT@5" direction="pwr"/>
<pin name="VOUT@6" direction="pwr"/>
<pin name="VOUT@7" direction="pwr"/>
<pin name="VOUT@8" direction="pwr"/>
<pin name="VOUT@9" direction="pwr"/>
<pin name="VOUT@10" direction="pwr"/>
<pin name="VOUT@11" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
</symbol>
<symbol name="LT1963EFE">
<pin name="IN@1" direction="in"/>
<pin name="OUT@1" direction="out"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="IN@2" direction="in"/>
<pin name="IN@3" direction="in"/>
<pin name="OUT@2" direction="out"/>
<pin name="OUT@3" direction="out"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="LT1763">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="BYP" direction="in"/>
</symbol>
<symbol name="LT1763DE">
<pin name="IN@1" direction="in"/>
<pin name="OUT@1" direction="pas"/>
<pin name="!SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="BYP" direction="in"/>
<pin name="IN@2" direction="in"/>
<pin name="OUT@2" direction="pas"/>
<pin name="EXP" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="V+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP-EN">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!EN"/>
</symbol>
<symbol name="LT5598">
<pin name="RF" direction="out"/>
<pin name="BBPI" direction="in"/>
<pin name="BBMI" direction="in"/>
<pin name="BBPQ" direction="in"/>
<pin name="BBMQ" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GNDRF@1" direction="pwr"/>
<pin name="GNDRF@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="LOP" direction="in"/>
<pin name="LOM" direction="in"/>
<pin name="CAPA" direction="in"/>
<pin name="CAPB" direction="in"/>
</symbol>
<symbol name="LT3539">
<pin name="VIN"/>
<pin name="MODE"/>
<pin name="!SHDN"/>
<pin name="GND"/>
<pin name="PGND"/>
<pin name="FB"/>
<pin name="VOUT"/>
<pin name="SW"/>
<pin name="PAD"/>
</symbol>
<symbol name="LT3991">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="PG"/>
<pin name="SS"/>
<pin name="SYNC"/>
<pin name="GND"/>
<pin name="BD"/>
<pin name="SW"/>
<pin name="BOOST"/>
<pin name="RT"/>
<pin name="FB"/>
</symbol>
<symbol name="LT3684">
<pin name="VIN"/>
<pin name="RUN/SS"/>
<pin name="PG"/>
<pin name="VC"/>
<pin name="BIAS"/>
<pin name="GND"/>
<pin name="BD"/>
<pin name="SW"/>
<pin name="BOOST"/>
<pin name="RT"/>
<pin name="FB"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LT1129CQ-5" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CS8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="NC" symbol="NC"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G2" pin="GND" pad="7"/>
<connect gate="NC" pin="NC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CT-5" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
</gates>
<devices>
<device name="" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CST5" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129-3"/>
<gate name="GND" symbol="GND"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="GND" pin="GND" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1016" prefix="IC" uservalue="yes">
<description>Ultra-fast precision &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LT1016"/>
</gates>
<devices>
<device name="CS8" package="SOIC8">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LA_EN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CN" package="DIL08">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LA_EN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1658MS8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LTC1658"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="!CSLD" pad="3"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1709-7" prefix="IC">
<description>&lt;b&gt;Synchronous Step-Down Switching Regulator&lt;/b&gt;&lt;p&gt;
2-Phase, 5-Bit VID, Current Mode, High Efficiency&lt;br&gt;
Source: www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1143,C1083,P1964,D1133</description>
<gates>
<gate name="G$1" symbol="LTC1709-7"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="ATTENIN" pad="16"/>
<connect gate="G$1" pin="ATTENOUT" pad="15"/>
<connect gate="G$1" pin="BG1" pad="31"/>
<connect gate="G$1" pin="BG2" pad="27"/>
<connect gate="G$1" pin="BOOST1" pad="33"/>
<connect gate="G$1" pin="BOOST2" pad="26"/>
<connect gate="G$1" pin="EAIN" pad="4"/>
<connect gate="G$1" pin="EXTVCC" pad="30"/>
<connect gate="G$1" pin="FCB" pad="7"/>
<connect gate="G$1" pin="INTVCC" pad="29"/>
<connect gate="G$1" pin="ITH" pad="8"/>
<connect gate="G$1" pin="NC" pad="36"/>
<connect gate="G$1" pin="PGND" pad="28"/>
<connect gate="G$1" pin="PGOOD" pad="23"/>
<connect gate="G$1" pin="PLLFLTR" pad="5"/>
<connect gate="G$1" pin="PLLIN" pad="6"/>
<connect gate="G$1" pin="RUN/SS" pad="1"/>
<connect gate="G$1" pin="SENSE1+" pad="2"/>
<connect gate="G$1" pin="SENSE1-" pad="3"/>
<connect gate="G$1" pin="SENSE2+" pad="14"/>
<connect gate="G$1" pin="SENSE2-" pad="13"/>
<connect gate="G$1" pin="SGND" pad="9"/>
<connect gate="G$1" pin="SW1" pad="34"/>
<connect gate="G$1" pin="SW2" pad="25"/>
<connect gate="G$1" pin="TG1" pad="35"/>
<connect gate="G$1" pin="TG2" pad="24"/>
<connect gate="G$1" pin="VBIAS" pad="22"/>
<connect gate="G$1" pin="VDIFFOUT" pad="10"/>
<connect gate="G$1" pin="VID0" pad="17"/>
<connect gate="G$1" pin="VID1" pad="18"/>
<connect gate="G$1" pin="VID2" pad="19"/>
<connect gate="G$1" pin="VID3" pad="20"/>
<connect gate="G$1" pin="VID4" pad="21"/>
<connect gate="G$1" pin="VIN" pad="32"/>
<connect gate="G$1" pin="VOS+" pad="12"/>
<connect gate="G$1" pin="VOS-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4062" prefix="IC">
<description>&lt;b&gt;Standalone Linear Li-Ion Battery Charger with Micropower Comparator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. 4062fa.pdf</description>
<gates>
<gate name="G$1" symbol="LTC4062"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="!C/5" pad="6"/>
<connect gate="G$1" pin="!CHRG" pad="5"/>
<connect gate="G$1" pin="!EN" pad="7"/>
<connect gate="G$1" pin="BAT" pad="1"/>
<connect gate="G$1" pin="GND" pad="EXP"/>
<connect gate="G$1" pin="IDET" pad="8"/>
<connect gate="G$1" pin="IN+" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="PROG" pad="9"/>
<connect gate="G$1" pin="TIMER" pad="3"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC128*C" prefix="IC">
<description>&lt;b&gt;3V Micropower Sampling 12-Bit A/D Converters&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1155,C1001,C1158,P1489,D3463</description>
<gates>
<gate name="G$1" symbol="LTC1288"/>
</gates>
<devices>
<device name="S8" package="SOIC8">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN/C0" pad="2"/>
<connect gate="G$1" pin="-IN/C1" pad="3"/>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="5"/>
<technology name="8"/>
</technologies>
</device>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN/C0" pad="2"/>
<connect gate="G$1" pin="-IN/C1" pad="3"/>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="5"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC26*" prefix="IC">
<description>&lt;b&gt;Dual 16-/14-/12-Bit Rail-to-Rail DACs&lt;/b&gt;&lt;p&gt;
Source: www.linear.com</description>
<gates>
<gate name="-1" symbol="LTC2602"/>
</gates>
<devices>
<device name="MS8" package="MSOP8">
<connects>
<connect gate="-1" pin="!CS/LD" pad="1"/>
<connect gate="-1" pin="GND" pad="7"/>
<connect gate="-1" pin="REF" pad="4"/>
<connect gate="-1" pin="SCK" pad="2"/>
<connect gate="-1" pin="SDI" pad="3"/>
<connect gate="-1" pin="VCC" pad="6"/>
<connect gate="-1" pin="VOUTA" pad="8"/>
<connect gate="-1" pin="VOUTB" pad="5"/>
</connects>
<technologies>
<technology name="02C"/>
<technology name="02I"/>
<technology name="12C"/>
<technology name="12I"/>
<technology name="22C"/>
<technology name="22I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1535*" prefix="IC">
<description>&lt;b&gt;Isolated RS485 Transceiver&lt;/b&gt;&lt;p&gt;
Source : www.linear.com</description>
<gates>
<gate name="-1" symbol="LTC1535"/>
</gates>
<devices>
<device name="SW" package="SO28SW">
<connects>
<connect gate="-1" pin="!RE" pad="27"/>
<connect gate="-1" pin="!SLO" pad="18"/>
<connect gate="-1" pin="A" pad="16"/>
<connect gate="-1" pin="B" pad="15"/>
<connect gate="-1" pin="DE" pad="26"/>
<connect gate="-1" pin="DI" pad="25"/>
<connect gate="-1" pin="GND" pad="4"/>
<connect gate="-1" pin="GND2" pad="11"/>
<connect gate="-1" pin="RO" pad="28"/>
<connect gate="-1" pin="RO2" pad="17"/>
<connect gate="-1" pin="ST1" pad="2"/>
<connect gate="-1" pin="ST2" pad="3"/>
<connect gate="-1" pin="VCC" pad="1"/>
<connect gate="-1" pin="VCC2" pad="14"/>
<connect gate="-1" pin="Y" pad="13"/>
<connect gate="-1" pin="Z" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC485" prefix="IC">
<description>&lt;b&gt;Low Power RS485 Interface Transceiver&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1007,C1017,P2064,D1718</description>
<gates>
<gate name="G$1" symbol="LTC485"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963AEQ*" prefix="IC">
<description>&lt;b&gt;LT1963 1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com</description>
<gates>
<gate name="A" symbol="LT1963"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="A" pin="!SHDN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND@1" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963AET*" prefix="IC">
<description>&lt;b&gt;LT1963 1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com</description>
<gates>
<gate name="G$1" symbol="LT1963ET"/>
</gates>
<devices>
<device name="" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1021" prefix="IC">
<description>&lt;b&gt;Precision Reference&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1010,C1603,P1229,D2805</description>
<gates>
<gate name="G$1" symbol="LT1021"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3549" prefix="IC">
<description>&lt;b&gt;250mA Low VIN Buck&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1032,C1063,P26952,D16357</description>
<gates>
<gate name="G$1" symbol="LTC3549"/>
</gates>
<devices>
<device name="" package="DFN6-2X3">
<connects>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="MODE" pad="4"/>
<connect gate="G$1" pin="RUN" pad="5"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="VFB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3681" prefix="IC">
<description>36V, 2A, 2.8MHz &lt;b&gt;Step-Down Switching Regulator&lt;/b&gt; with Integrated Power Schottky Diode&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1032,C1064,P38040,D25144</description>
<gates>
<gate name="G$1" symbol="LT3681"/>
</gates>
<devices>
<device name="" package="DFN14-4X3DE">
<connects>
<connect gate="G$1" pin="BD" pad="10"/>
<connect gate="G$1" pin="BIAS" pad="2"/>
<connect gate="G$1" pin="BOOST" pad="11"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DC" pad="9"/>
<connect gate="G$1" pin="DC@1" pad="9@2"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="4@1"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="PG" pad="1"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="RUN/SS" pad="14"/>
<connect gate="G$1" pin="SW" pad="12"/>
<connect gate="G$1" pin="VC" pad="5"/>
<connect gate="G$1" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1168" prefix="IC">
<description>&lt;b&gt;Low Power, Single Resistor Gain Programmable, Precision Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
SourcE: LT1168.pdf</description>
<gates>
<gate name="P" symbol="LT1168"/>
</gates>
<devices>
<device name="N8" package="DIL08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="REF" pad="5"/>
<connect gate="P" pin="RG@1" pad="1"/>
<connect gate="P" pin="RG@2" pad="8"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="AI"/>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
<device name="S8" package="SOIC8">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="REF" pad="5"/>
<connect gate="P" pin="RG@1" pad="1"/>
<connect gate="P" pin="RG@2" pad="8"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="AI"/>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1236?*" prefix="IC">
<description>&lt;b&gt;Precision Voltage Reference&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1154,C1002,C1243,P1156,D2948</description>
<gates>
<gate name="G$1" symbol="LT1236"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-5"/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-5"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1019?*" prefix="IC">
<description>&lt;b&gt;Precision Voltage Reference&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1154,C1002,C1243,P1130,D3834</description>
<gates>
<gate name="G$1" symbol="LT1236"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-2.5"/>
<technology name="-4.5"/>
<technology name="-5"/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1257" prefix="IC">
<description>&lt;b&gt;Complete Single Supply 12-Bit Voltage Output DAC&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1155,C1005,C1156,P1425,D3414</description>
<gates>
<gate name="G$1" symbol="LT1257"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!LOAD" pad="3"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="!LOAD" pad="3"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963E" prefix="IC">
<description>&lt;b&gt;1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C3,P2222,D3148</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
</gates>
<devices>
<device name="Q" package="Q5-DD">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
<device name="T" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963ES8" prefix="IC">
<description>&lt;b&gt;1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C3,P2222,D3148</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="NC" symbol="NC"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G2" pin="GND" pad="7"/>
<connect gate="NC" pin="NC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963EST" prefix="IC">
<description>&lt;b&gt;1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C3,P2222,D3148</description>
<gates>
<gate name="G$1" symbol="LT1129-3"/>
<gate name="G$2" symbol="GND"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$2" pin="GND" pad="4"/>
</connects>
<technologies>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3611" prefix="IC">
<description>&lt;b&gt;10A, 32V Monolithic Synchronous Step-Down DC/DC Converter&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com ..</description>
<gates>
<gate name="G$1" symbol="LTC3610"/>
<gate name="P" symbol="LTC3610-P"/>
</gates>
<devices>
<device name="" package="QFN64-9X9">
<connects>
<connect gate="G$1" pin="BOOST" pad="29"/>
<connect gate="G$1" pin="EXTVCC" pad="44"/>
<connect gate="G$1" pin="FCB" pad="39"/>
<connect gate="G$1" pin="INTVCC@1" pad="53"/>
<connect gate="G$1" pin="INTVCC@2" pad="54"/>
<connect gate="G$1" pin="ION" pad="41"/>
<connect gate="G$1" pin="ITH" pad="38"/>
<connect gate="G$1" pin="PGND@1" pad="1"/>
<connect gate="G$1" pin="PGND@10" pad="62"/>
<connect gate="G$1" pin="PGND@11" pad="63"/>
<connect gate="G$1" pin="PGND@12" pad="64"/>
<connect gate="G$1" pin="PGND@13" pad="65"/>
<connect gate="G$1" pin="PGND@2" pad="2"/>
<connect gate="G$1" pin="PGND@3" pad="3"/>
<connect gate="G$1" pin="PGND@4" pad="56"/>
<connect gate="G$1" pin="PGND@5" pad="57"/>
<connect gate="G$1" pin="PGND@6" pad="58"/>
<connect gate="G$1" pin="PGND@7" pad="59"/>
<connect gate="G$1" pin="PGND@8" pad="60"/>
<connect gate="G$1" pin="PGND@9" pad="61"/>
<connect gate="G$1" pin="PGOOD" pad="36"/>
<connect gate="G$1" pin="PVIN@1" pad="12"/>
<connect gate="G$1" pin="PVIN@10" pad="21"/>
<connect gate="G$1" pin="PVIN@11" pad="22"/>
<connect gate="G$1" pin="PVIN@12" pad="23"/>
<connect gate="G$1" pin="PVIN@13" pad="24"/>
<connect gate="G$1" pin="PVIN@14" pad="25"/>
<connect gate="G$1" pin="PVIN@15" pad="67"/>
<connect gate="G$1" pin="PVIN@2" pad="13"/>
<connect gate="G$1" pin="PVIN@3" pad="14"/>
<connect gate="G$1" pin="PVIN@4" pad="15"/>
<connect gate="G$1" pin="PVIN@5" pad="16"/>
<connect gate="G$1" pin="PVIN@6" pad="17"/>
<connect gate="G$1" pin="PVIN@7" pad="18"/>
<connect gate="G$1" pin="PVIN@8" pad="19"/>
<connect gate="G$1" pin="PVIN@9" pad="20"/>
<connect gate="G$1" pin="RUN/SS" pad="30"/>
<connect gate="G$1" pin="SGND@1" pad="28"/>
<connect gate="G$1" pin="SGND@10" pad="47"/>
<connect gate="G$1" pin="SGND@11" pad="48"/>
<connect gate="G$1" pin="SGND@12" pad="49"/>
<connect gate="G$1" pin="SGND@13" pad="50"/>
<connect gate="G$1" pin="SGND@2" pad="31"/>
<connect gate="G$1" pin="SGND@3" pad="32"/>
<connect gate="G$1" pin="SGND@4" pad="33"/>
<connect gate="G$1" pin="SGND@5" pad="34"/>
<connect gate="G$1" pin="SGND@6" pad="40"/>
<connect gate="G$1" pin="SGND@7" pad="42"/>
<connect gate="G$1" pin="SGND@8" pad="45"/>
<connect gate="G$1" pin="SGND@9" pad="46"/>
<connect gate="G$1" pin="SVIN@1" pad="51"/>
<connect gate="G$1" pin="SVIN@2" pad="52"/>
<connect gate="G$1" pin="SW@1" pad="4"/>
<connect gate="G$1" pin="SW@10" pad="55"/>
<connect gate="G$1" pin="SW@11" pad="66"/>
<connect gate="G$1" pin="SW@2" pad="5"/>
<connect gate="G$1" pin="SW@3" pad="6"/>
<connect gate="G$1" pin="SW@4" pad="7"/>
<connect gate="G$1" pin="SW@5" pad="8"/>
<connect gate="G$1" pin="SW@6" pad="9"/>
<connect gate="G$1" pin="SW@7" pad="10"/>
<connect gate="G$1" pin="SW@8" pad="11"/>
<connect gate="G$1" pin="SW@9" pad="26"/>
<connect gate="G$1" pin="VFB" pad="43"/>
<connect gate="G$1" pin="VON" pad="35"/>
<connect gate="G$1" pin="VRNG" pad="37"/>
<connect gate="P" pin="INTVCC@1" pad="53@1"/>
<connect gate="P" pin="INTVCC@2" pad="53@2"/>
<connect gate="P" pin="INTVCC@3" pad="53@3"/>
<connect gate="P" pin="INTVCC@4" pad="53@4"/>
<connect gate="P" pin="INTVCC@5" pad="54@1"/>
<connect gate="P" pin="SGND@1" pad="68"/>
<connect gate="P" pin="SVIN@1" pad="51@1"/>
<connect gate="P" pin="SVIN@2" pad="51@2"/>
<connect gate="P" pin="SVIN@3" pad="51@3"/>
<connect gate="P" pin="SVIN@4" pad="51@4"/>
<connect gate="P" pin="SVIN@5" pad="51@5"/>
<connect gate="P" pin="SVIN@6" pad="52@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1996" prefix="IC">
<description>&lt;b&gt;Precision, 100µA Gain Selectable Amplifier&lt;/b&gt;&lt;p&gt;
Difference Amplifier, Gain Range 9 to 117, CMRR &gt;80dB&lt;br&gt;
Source: http://www.linear.com</description>
<gates>
<gate name="G$1" symbol="LT1996"/>
</gates>
<devices>
<device name="DD" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="M27" pad="9"/>
<connect gate="G$1" pin="M81" pad="8"/>
<connect gate="G$1" pin="M9" pad="10"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="P27" pad="2"/>
<connect gate="G$1" pin="P81" pad="3"/>
<connect gate="G$1" pin="P9" pad="1"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="AI"/>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
<device name="MS" package="MSOP10">
<connects>
<connect gate="G$1" pin="M27" pad="9"/>
<connect gate="G$1" pin="M81" pad="8"/>
<connect gate="G$1" pin="M9" pad="10"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="P27" pad="2"/>
<connect gate="G$1" pin="P81" pad="3"/>
<connect gate="G$1" pin="P9" pad="1"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="AI"/>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3610" prefix="IC">
<description>&lt;b&gt;12A, 24V Monolithic Synchronous Step-Down DC/DC Converter&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com ..</description>
<gates>
<gate name="G$1" symbol="LTC3610"/>
<gate name="P" symbol="LTC3610-P"/>
</gates>
<devices>
<device name="" package="QFN64-9X9">
<connects>
<connect gate="G$1" pin="BOOST" pad="29"/>
<connect gate="G$1" pin="EXTVCC" pad="44"/>
<connect gate="G$1" pin="FCB" pad="39"/>
<connect gate="G$1" pin="INTVCC@1" pad="53"/>
<connect gate="G$1" pin="INTVCC@2" pad="54"/>
<connect gate="G$1" pin="ION" pad="41"/>
<connect gate="G$1" pin="ITH" pad="38"/>
<connect gate="G$1" pin="PGND@1" pad="1"/>
<connect gate="G$1" pin="PGND@10" pad="62"/>
<connect gate="G$1" pin="PGND@11" pad="63"/>
<connect gate="G$1" pin="PGND@12" pad="64"/>
<connect gate="G$1" pin="PGND@13" pad="65"/>
<connect gate="G$1" pin="PGND@2" pad="2"/>
<connect gate="G$1" pin="PGND@3" pad="3"/>
<connect gate="G$1" pin="PGND@4" pad="56"/>
<connect gate="G$1" pin="PGND@5" pad="57"/>
<connect gate="G$1" pin="PGND@6" pad="58"/>
<connect gate="G$1" pin="PGND@7" pad="59"/>
<connect gate="G$1" pin="PGND@8" pad="60"/>
<connect gate="G$1" pin="PGND@9" pad="61"/>
<connect gate="G$1" pin="PGOOD" pad="36"/>
<connect gate="G$1" pin="PVIN@1" pad="12"/>
<connect gate="G$1" pin="PVIN@10" pad="21"/>
<connect gate="G$1" pin="PVIN@11" pad="22"/>
<connect gate="G$1" pin="PVIN@12" pad="23"/>
<connect gate="G$1" pin="PVIN@13" pad="24"/>
<connect gate="G$1" pin="PVIN@14" pad="25"/>
<connect gate="G$1" pin="PVIN@15" pad="67"/>
<connect gate="G$1" pin="PVIN@2" pad="13"/>
<connect gate="G$1" pin="PVIN@3" pad="14"/>
<connect gate="G$1" pin="PVIN@4" pad="15"/>
<connect gate="G$1" pin="PVIN@5" pad="16"/>
<connect gate="G$1" pin="PVIN@6" pad="17"/>
<connect gate="G$1" pin="PVIN@7" pad="18"/>
<connect gate="G$1" pin="PVIN@8" pad="19"/>
<connect gate="G$1" pin="PVIN@9" pad="20"/>
<connect gate="G$1" pin="RUN/SS" pad="30"/>
<connect gate="G$1" pin="SGND@1" pad="28"/>
<connect gate="G$1" pin="SGND@10" pad="47"/>
<connect gate="G$1" pin="SGND@11" pad="48"/>
<connect gate="G$1" pin="SGND@12" pad="49"/>
<connect gate="G$1" pin="SGND@13" pad="50"/>
<connect gate="G$1" pin="SGND@2" pad="31"/>
<connect gate="G$1" pin="SGND@3" pad="32"/>
<connect gate="G$1" pin="SGND@4" pad="33"/>
<connect gate="G$1" pin="SGND@5" pad="34"/>
<connect gate="G$1" pin="SGND@6" pad="40"/>
<connect gate="G$1" pin="SGND@7" pad="42"/>
<connect gate="G$1" pin="SGND@8" pad="45"/>
<connect gate="G$1" pin="SGND@9" pad="46"/>
<connect gate="G$1" pin="SVIN@1" pad="51"/>
<connect gate="G$1" pin="SVIN@2" pad="52"/>
<connect gate="G$1" pin="SW@1" pad="4"/>
<connect gate="G$1" pin="SW@10" pad="55"/>
<connect gate="G$1" pin="SW@11" pad="66"/>
<connect gate="G$1" pin="SW@2" pad="5"/>
<connect gate="G$1" pin="SW@3" pad="6"/>
<connect gate="G$1" pin="SW@4" pad="7"/>
<connect gate="G$1" pin="SW@5" pad="8"/>
<connect gate="G$1" pin="SW@6" pad="9"/>
<connect gate="G$1" pin="SW@7" pad="10"/>
<connect gate="G$1" pin="SW@8" pad="11"/>
<connect gate="G$1" pin="SW@9" pad="26"/>
<connect gate="G$1" pin="VFB" pad="43"/>
<connect gate="G$1" pin="VON" pad="35"/>
<connect gate="G$1" pin="VRNG" pad="37"/>
<connect gate="P" pin="INTVCC@1" pad="53@1"/>
<connect gate="P" pin="INTVCC@2" pad="53@2"/>
<connect gate="P" pin="INTVCC@3" pad="53@3"/>
<connect gate="P" pin="INTVCC@4" pad="53@4"/>
<connect gate="P" pin="INTVCC@5" pad="54@1"/>
<connect gate="P" pin="SGND@1" pad="68"/>
<connect gate="P" pin="SVIN@1" pad="51@1"/>
<connect gate="P" pin="SVIN@2" pad="51@2"/>
<connect gate="P" pin="SVIN@3" pad="51@3"/>
<connect gate="P" pin="SVIN@4" pad="51@4"/>
<connect gate="P" pin="SVIN@5" pad="51@5"/>
<connect gate="P" pin="SVIN@6" pad="52@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2486" prefix="IC">
<description>&lt;b&gt;16-Bit 2-/4-Channel Delta Sigma ADC&lt;/b&gt;&lt;p&gt;
with PGA and Easy Drive Input Current Cancellation&lt;br&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1155,C1001,C1152,P36532,D19318</description>
<gates>
<gate name="G$1" symbol="LTC2486"/>
</gates>
<devices>
<device name="" package="DFN14-4X3">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="CH0" pad="8"/>
<connect gate="G$1" pin="CH1" pad="9"/>
<connect gate="G$1" pin="CH2" pad="10"/>
<connect gate="G$1" pin="CH3" pad="11"/>
<connect gate="G$1" pin="COM" pad="7"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FO" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VREF+" pad="13"/>
<connect gate="G$1" pin="VREF-" pad="14"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2482" prefix="IC">
<description>&lt;b&gt;16-Bit Delta Sigma ADC with Easy Drive Input Current Cancellation&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1155,C1001,C1152,P11253,D7998</description>
<gates>
<gate name="G$1" symbol="LTC2482"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FO" pad="10"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@*" pad="1"/>
<connect gate="G$1" pin="IN+" pad="4"/>
<connect gate="G$1" pin="IN-" pad="5"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SDO" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VREF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTM8023" prefix="IC">
<description>&lt;b&gt;2A, 36V DC/DC µModule&lt;p&gt;
Complete Step-Down Switch Mode Power Supply&lt;br&gt;
Source: http://www.linear.com .. 8023fc.pdf</description>
<gates>
<gate name="G$1" symbol="LTM8023"/>
<gate name="P" symbol="LTM8023-P"/>
</gates>
<devices>
<device name="" package="LGA50">
<connects>
<connect gate="G$1" pin="ADJ" pad="H7"/>
<connect gate="G$1" pin="AUX" pad="F5"/>
<connect gate="G$1" pin="BIAS" pad="G5"/>
<connect gate="G$1" pin="GND" pad="D1"/>
<connect gate="G$1" pin="PGOOD" pad="H6"/>
<connect gate="G$1" pin="RT" pad="G7"/>
<connect gate="G$1" pin="RUN/SS" pad="H5"/>
<connect gate="G$1" pin="SHARE" pad="F7"/>
<connect gate="G$1" pin="SYNC" pad="G6"/>
<connect gate="G$1" pin="VIN" pad="H1"/>
<connect gate="G$1" pin="VOUT" pad="A1"/>
<connect gate="P" pin="GND@1" pad="D2"/>
<connect gate="P" pin="GND@10" pad="E5"/>
<connect gate="P" pin="GND@11" pad="E6"/>
<connect gate="P" pin="GND@12" pad="E7"/>
<connect gate="P" pin="GND@13" pad="F6"/>
<connect gate="P" pin="GND@14" pad="A5"/>
<connect gate="P" pin="GND@15" pad="A6"/>
<connect gate="P" pin="GND@16" pad="A7"/>
<connect gate="P" pin="GND@17" pad="B5"/>
<connect gate="P" pin="GND@18" pad="B6"/>
<connect gate="P" pin="GND@19" pad="B7"/>
<connect gate="P" pin="GND@2" pad="D3"/>
<connect gate="P" pin="GND@20" pad="C5"/>
<connect gate="P" pin="GND@21" pad="C6"/>
<connect gate="P" pin="GND@22" pad="C7"/>
<connect gate="P" pin="GND@23" pad="D7"/>
<connect gate="P" pin="GND@3" pad="D4"/>
<connect gate="P" pin="GND@4" pad="D5"/>
<connect gate="P" pin="GND@5" pad="D6"/>
<connect gate="P" pin="GND@6" pad="E1"/>
<connect gate="P" pin="GND@7" pad="E2"/>
<connect gate="P" pin="GND@8" pad="E3"/>
<connect gate="P" pin="GND@9" pad="E4"/>
<connect gate="P" pin="VIN@1" pad="G1"/>
<connect gate="P" pin="VIN@2" pad="G2"/>
<connect gate="P" pin="VIN@3" pad="G3"/>
<connect gate="P" pin="VIN@4" pad="H2"/>
<connect gate="P" pin="VIN@5" pad="H3"/>
<connect gate="P" pin="VOUT@1" pad="A2"/>
<connect gate="P" pin="VOUT@10" pad="C3"/>
<connect gate="P" pin="VOUT@11" pad="C4"/>
<connect gate="P" pin="VOUT@2" pad="A3"/>
<connect gate="P" pin="VOUT@3" pad="A4"/>
<connect gate="P" pin="VOUT@4" pad="B1"/>
<connect gate="P" pin="VOUT@5" pad="B2"/>
<connect gate="P" pin="VOUT@6" pad="B3"/>
<connect gate="P" pin="VOUT@7" pad="B4"/>
<connect gate="P" pin="VOUT@8" pad="C1"/>
<connect gate="P" pin="VOUT@9" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963EFE" prefix="IC">
<description>&lt;b&gt;1.5A, Low Noise, Fast Transient Response LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/1963fc.pdf</description>
<gates>
<gate name="G$1" symbol="LT1963EFE"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!SHDN" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="8"/>
<connect gate="G$1" pin="GND@4" pad="9"/>
<connect gate="G$1" pin="GND@5" pad="15"/>
<connect gate="G$1" pin="IN@1" pad="14"/>
<connect gate="G$1" pin="IN@2" pad="13"/>
<connect gate="G$1" pin="IN@3" pad="12"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="OUT@3" pad="5"/>
<connect gate="G$1" pin="SENSE" pad="6"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1763CS8" prefix="IC">
<description>&lt;b&gt;500mA, Low Noise, LDO Micropower Regulators&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/1763ff.pdf</description>
<gates>
<gate name="G$1" symbol="LT1763"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="7"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name="-1.5"/>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3"/>
<technology name="-3.3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1763" prefix="IC">
<description>&lt;b&gt;500mA, Low Noise, LDO Micropower Regulators&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/1763ff.pdf</description>
<gates>
<gate name="G$1" symbol="LT1763DE"/>
</gates>
<devices>
<device name="" package="DFN12">
<connects>
<connect gate="G$1" pin="!SHDN" pad="8"/>
<connect gate="G$1" pin="BYP" pad="6"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN@1" pad="11"/>
<connect gate="G$1" pin="IN@2" pad="10"/>
<connect gate="G$1" pin="OUT@1" pad="2"/>
<connect gate="G$1" pin="OUT@2" pad="3"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
</connects>
<technologies>
<technology name="CDE"/>
<technology name="CDE-1.5"/>
<technology name="CDE-1.8"/>
<technology name="CDE-2.5"/>
<technology name="CDE-3"/>
<technology name="CDE-3.3"/>
<technology name="CDE-5"/>
<technology name="IDE"/>
<technology name="IDE-1.5"/>
<technology name="IDE-1.8"/>
<technology name="IDE-2.5"/>
<technology name="IDE-3"/>
<technology name="IDE-3.3"/>
<technology name="IDE-5"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT6231" prefix="IC">
<description>&lt;b&gt;215MHz, Rail-to-Rail Output, 1.1nV/Hz, 3.5mA Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="V+-"/>
</gates>
<devices>
<device name="S8" package="S8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
<device name="DD" package="DFN8-3X3">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT6230" prefix="IC">
<description>&lt;b&gt;215MHz, Rail-to-Rail Output, 1.1nV/Hz, 3.5mA Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
<gates>
<gate name="A" symbol="OPAMP-EN"/>
<gate name="B" symbol="V+-"/>
</gates>
<devices>
<device name="" package="TSOT23-6">
<connects>
<connect gate="A" pin="!EN" pad="5"/>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="V+" pad="6"/>
<connect gate="B" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="CS6"/>
<technology name="CS6-10"/>
<technology name="IS6"/>
<technology name="IS6-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT6232" prefix="IC">
<description>&lt;b&gt;215MHz, Rail-to-Rail Output, 1.1nV/Hz, 3.5mA Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="V+-"/>
</gates>
<devices>
<device name="GN" package="SSOP16">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT5598" prefix="IC">
<description>&lt;b&gt;5MHz to 1600MHz High Linearity Direct Quadrature Modulator&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/5598f.pdf</description>
<gates>
<gate name="P" symbol="LT5598"/>
</gates>
<devices>
<device name="UF" package="QFN24-4X4">
<connects>
<connect gate="P" pin="BBMI" pad="22"/>
<connect gate="P" pin="BBMQ" pad="9"/>
<connect gate="P" pin="BBPI" pad="21"/>
<connect gate="P" pin="BBPQ" pad="10"/>
<connect gate="P" pin="CAPA" pad="6"/>
<connect gate="P" pin="CAPB" pad="7"/>
<connect gate="P" pin="EN" pad="1"/>
<connect gate="P" pin="GND@1" pad="2"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="11"/>
<connect gate="P" pin="GND@5" pad="12"/>
<connect gate="P" pin="GND@6" pad="19"/>
<connect gate="P" pin="GND@7" pad="20"/>
<connect gate="P" pin="GND@8" pad="23"/>
<connect gate="P" pin="GNDRF@1" pad="14"/>
<connect gate="P" pin="GNDRF@2" pad="17"/>
<connect gate="P" pin="LOM" pad="4"/>
<connect gate="P" pin="LOP" pad="3"/>
<connect gate="P" pin="RF" pad="16"/>
<connect gate="P" pin="VCC@1" pad="24"/>
<connect gate="P" pin="VCC@2" pad="18"/>
</connects>
<technologies>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3539">
<gates>
<gate name="G$1" symbol="LT3539"/>
</gates>
<devices>
<device name="" package="DFN8-2X3">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="PAD" pad="EXP"/>
<connect gate="G$1" pin="PGND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3991">
<gates>
<gate name="G$1" symbol="LT3991"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="BD" pad="1"/>
<connect gate="G$1" pin="BOOST" pad="2"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="EXP"/>
<connect gate="G$1" pin="PG" pad="9"/>
<connect gate="G$1" pin="RT" pad="8"/>
<connect gate="G$1" pin="SS" pad="7"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3684">
<gates>
<gate name="G$1" symbol="LT3684"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="BD" pad="1"/>
<connect gate="G$1" pin="BIAS" pad="7"/>
<connect gate="G$1" pin="BOOST" pad="2"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="GND" pad="EXP"/>
<connect gate="G$1" pin="PG" pad="6"/>
<connect gate="G$1" pin="RT" pad="10"/>
<connect gate="G$1" pin="RUN/SS" pad="5"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="VC" pad="9"/>
<connect gate="G$1" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
