<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>5V CPLD w/ISP 

32 Macrocell, low power w/ISP, 5V</description>
<packages>
<package name="3M44">
<description>&lt;b&gt;PLCC SOCKET&lt;/b&gt;</description>
</package>
<package name="PQFP-100">
<description>PQFP100
Quad flat pack 14mm x 20mm</description>
</package>
<package name="TQFP-100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
<package name="S84">
<description>&lt;b&gt;84 Pin PLCC Socket&lt;/b&gt;</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="TH-100">
<description>Through-hole adapter mounted pqfp-100 part.</description>
</package>
<package name="TH100B">
<description>Experimental 100 pin PQFP "pachage".</description>
</package>
</packages>
<symbols>
<symbol name="ATF1502ASL">
<pin name="GCLR_IN"/>
<pin name="GCLK2_OE2_IN"/>
<pin name="GCLK1_IN"/>
<pin name="I/O_0"/>
<pin name="I/O_1"/>
<pin name="I/O_2"/>
<pin name="TDI_I/O_3"/>
<pin name="VCC0"/>
<pin name="I/O_4"/>
<pin name="I/O_5"/>
<pin name="PD1_I/O_6"/>
<pin name="I/O_7"/>
<pin name="TMS_I/O_8"/>
<pin name="I/O_9"/>
<pin name="GND0"/>
<pin name="VCC1"/>
<pin name="I/O_10"/>
<pin name="I/O_11"/>
<pin name="I/O_12"/>
<pin name="I/O_13"/>
<pin name="I/0_14"/>
<pin name="I/0_15"/>
<pin name="GND1"/>
<pin name="VCC2"/>
<pin name="I/0_16"/>
<pin name="PD2_I/O_17"/>
<pin name="I/O_18"/>
<pin name="I/O_19"/>
<pin name="I/O_20"/>
<pin name="I/O_21"/>
<pin name="I/O_22"/>
<pin name="TCK_I/O_23"/>
<pin name="I/O_24"/>
<pin name="I/O_25"/>
<pin name="I/O_26"/>
<pin name="I/O_27"/>
<pin name="TDO_I/O_28"/>
<pin name="I/O_29"/>
<pin name="I/0_30"/>
<pin name="GCLK3_I/O_31"/>
<pin name="GND2"/>
<pin name="VCC3"/>
<pin name="GND3"/>
<pin name="OE1_IN"/>
</symbol>
<symbol name="AT1508-100">
<pin name="IO/PD1"/>
<pin name="IO/PD2"/>
<pin name="IO/GCLK3"/>
<pin name="IN/GCLK1" direction="in"/>
<pin name="IN/OE1" direction="in"/>
<pin name="IN/GCLR" direction="in"/>
<pin name="IN/GCLK2/OE2" direction="in"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO66"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO74"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO73"/>
</symbol>
<symbol name="PVCCINT">
<pin name="VCCINT" direction="pwr"/>
</symbol>
<symbol name="PVCCIO">
<pin name="VCCIO" direction="pwr"/>
</symbol>
<symbol name="PGND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="JTAG">
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TDO"/>
</symbol>
<symbol name="AT1508-84">
<pin name="IO/PD1"/>
<pin name="IO/PD2"/>
<pin name="IO/GCLK3"/>
<pin name="IN/GCLK1" direction="in"/>
<pin name="IN/OE1" direction="in"/>
<pin name="IN/GCLR" direction="in"/>
<pin name="IN/GCLK2/OE2" direction="in"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO1"/>
</symbol>
<symbol name="AT1504-44">
<description>ATF150x in 44 pin packages</description>
<pin name="IN/GCLR" direction="in"/>
<pin name="IN/OE2/GCLK2" direction="in"/>
<pin name="IN/GCLK1" direction="in"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO1/TDI"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO4/PD1"/>
<pin name="IO9"/>
<pin name="IO6/TMS"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO18"/>
<pin name="IO17"/>
<pin name="IO15/PD2"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO21/TCK"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO30"/>
<pin name="IO26/TDO"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO29/GCLK3"/>
<pin name="IN/OE1" direction="in"/>
</symbol>
<symbol name="PVCC">
<pin name="VCC" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATF1502" uservalue="yes">
<description>ATF150x in 44 pin package.</description>
<gates>
<gate name="G$1" symbol="ATF1502ASL"/>
</gates>
<devices>
<device name="PLCC44" package="3M44">
<connects>
<connect gate="G$1" pin="GCLK1_IN" pad="43"/>
<connect gate="G$1" pin="GCLK2_OE2_IN" pad="2"/>
<connect gate="G$1" pin="GCLK3_I/O_31" pad="41"/>
<connect gate="G$1" pin="GCLR_IN" pad="1"/>
<connect gate="G$1" pin="GND0" pad="10"/>
<connect gate="G$1" pin="GND1" pad="22"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="42"/>
<connect gate="G$1" pin="I/0_14" pad="20"/>
<connect gate="G$1" pin="I/0_15" pad="21"/>
<connect gate="G$1" pin="I/0_16" pad="24"/>
<connect gate="G$1" pin="I/0_30" pad="40"/>
<connect gate="G$1" pin="I/O_0" pad="4"/>
<connect gate="G$1" pin="I/O_1" pad="5"/>
<connect gate="G$1" pin="I/O_10" pad="16"/>
<connect gate="G$1" pin="I/O_11" pad="17"/>
<connect gate="G$1" pin="I/O_12" pad="18"/>
<connect gate="G$1" pin="I/O_13" pad="19"/>
<connect gate="G$1" pin="I/O_18" pad="26"/>
<connect gate="G$1" pin="I/O_19" pad="27"/>
<connect gate="G$1" pin="I/O_2" pad="6"/>
<connect gate="G$1" pin="I/O_20" pad="28"/>
<connect gate="G$1" pin="I/O_21" pad="29"/>
<connect gate="G$1" pin="I/O_22" pad="31"/>
<connect gate="G$1" pin="I/O_24" pad="33"/>
<connect gate="G$1" pin="I/O_25" pad="34"/>
<connect gate="G$1" pin="I/O_26" pad="36"/>
<connect gate="G$1" pin="I/O_27" pad="37"/>
<connect gate="G$1" pin="I/O_29" pad="39"/>
<connect gate="G$1" pin="I/O_4" pad="8"/>
<connect gate="G$1" pin="I/O_5" pad="9"/>
<connect gate="G$1" pin="I/O_7" pad="12"/>
<connect gate="G$1" pin="I/O_9" pad="14"/>
<connect gate="G$1" pin="OE1_IN" pad="44"/>
<connect gate="G$1" pin="PD1_I/O_6" pad="11"/>
<connect gate="G$1" pin="PD2_I/O_17" pad="25"/>
<connect gate="G$1" pin="TCK_I/O_23" pad="32"/>
<connect gate="G$1" pin="TDI_I/O_3" pad="7"/>
<connect gate="G$1" pin="TDO_I/O_28" pad="38"/>
<connect gate="G$1" pin="TMS_I/O_8" pad="13"/>
<connect gate="G$1" pin="VCC0" pad="3"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2" pad="23"/>
<connect gate="G$1" pin="VCC3" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATF150X100" prefix="E">
<description>ATF150x in 100 pin package.</description>
<gates>
<gate name="JEDEC" symbol="JTAG"/>
<gate name="G$3" symbol="PVCCINT"/>
<gate name="G$4" symbol="PVCCINT"/>
<gate name="G$5" symbol="PVCCIO"/>
<gate name="G$6" symbol="PVCCIO"/>
<gate name="G$7" symbol="PVCCIO"/>
<gate name="G$8" symbol="PVCCIO"/>
<gate name="G$9" symbol="PVCCIO"/>
<gate name="G$10" symbol="PGND"/>
<gate name="G$11" symbol="PGND"/>
<gate name="G$12" symbol="PGND"/>
<gate name="G$13" symbol="PGND"/>
<gate name="G$14" symbol="PGND"/>
<gate name="G$1" symbol="PVCCIO"/>
<gate name="IO" symbol="AT1508-100"/>
<gate name="G$15" symbol="PGND"/>
<gate name="G$16" symbol="PGND"/>
<gate name="G$17" symbol="PGND"/>
</gates>
<devices>
<device name="TQFP" package="TQFP-100">
<connects>
<connect gate="G$1" pin="VCCIO" pad="82"/>
<connect gate="G$10" pin="GND" pad="11"/>
<connect gate="G$11" pin="GND" pad="26"/>
<connect gate="G$12" pin="GND" pad="38"/>
<connect gate="G$13" pin="GND" pad="43"/>
<connect gate="G$14" pin="GND" pad="59"/>
<connect gate="G$15" pin="GND" pad="74"/>
<connect gate="G$16" pin="GND" pad="86"/>
<connect gate="G$17" pin="GND" pad="95"/>
<connect gate="G$3" pin="VCCINT" pad="39"/>
<connect gate="G$4" pin="VCCINT" pad="91"/>
<connect gate="G$5" pin="VCCIO" pad="3"/>
<connect gate="G$6" pin="VCCIO" pad="18"/>
<connect gate="G$7" pin="VCCIO" pad="34"/>
<connect gate="G$8" pin="VCCIO" pad="51"/>
<connect gate="G$9" pin="VCCIO" pad="66"/>
<connect gate="IO" pin="IN/GCLK1" pad="87"/>
<connect gate="IO" pin="IN/GCLK2/OE2" pad="90"/>
<connect gate="IO" pin="IN/GCLR" pad="89"/>
<connect gate="IO" pin="IN/OE1" pad="88"/>
<connect gate="IO" pin="IO/GCLK3" pad="85"/>
<connect gate="IO" pin="IO/PD1" pad="1"/>
<connect gate="IO" pin="IO/PD2" pad="41"/>
<connect gate="IO" pin="IO10" pad="13"/>
<connect gate="IO" pin="IO11" pad="14"/>
<connect gate="IO" pin="IO12" pad="16"/>
<connect gate="IO" pin="IO13" pad="17"/>
<connect gate="IO" pin="IO14" pad="19"/>
<connect gate="IO" pin="IO15" pad="20"/>
<connect gate="IO" pin="IO16" pad="21"/>
<connect gate="IO" pin="IO17" pad="22"/>
<connect gate="IO" pin="IO18" pad="23"/>
<connect gate="IO" pin="IO19" pad="24"/>
<connect gate="IO" pin="IO2" pad="2"/>
<connect gate="IO" pin="IO20" pad="25"/>
<connect gate="IO" pin="IO21" pad="27"/>
<connect gate="IO" pin="IO22" pad="28"/>
<connect gate="IO" pin="IO23" pad="29"/>
<connect gate="IO" pin="IO24" pad="30"/>
<connect gate="IO" pin="IO25" pad="31"/>
<connect gate="IO" pin="IO26" pad="32"/>
<connect gate="IO" pin="IO27" pad="33"/>
<connect gate="IO" pin="IO28" pad="35"/>
<connect gate="IO" pin="IO29" pad="36"/>
<connect gate="IO" pin="IO3" pad="5"/>
<connect gate="IO" pin="IO30" pad="37"/>
<connect gate="IO" pin="IO31" pad="40"/>
<connect gate="IO" pin="IO33" pad="42"/>
<connect gate="IO" pin="IO34" pad="44"/>
<connect gate="IO" pin="IO35" pad="45"/>
<connect gate="IO" pin="IO36" pad="46"/>
<connect gate="IO" pin="IO37" pad="47"/>
<connect gate="IO" pin="IO38" pad="48"/>
<connect gate="IO" pin="IO39" pad="49"/>
<connect gate="IO" pin="IO4" pad="6"/>
<connect gate="IO" pin="IO40" pad="50"/>
<connect gate="IO" pin="IO41" pad="52"/>
<connect gate="IO" pin="IO42" pad="53"/>
<connect gate="IO" pin="IO43" pad="54"/>
<connect gate="IO" pin="IO44" pad="55"/>
<connect gate="IO" pin="IO45" pad="56"/>
<connect gate="IO" pin="IO46" pad="57"/>
<connect gate="IO" pin="IO47" pad="58"/>
<connect gate="IO" pin="IO48" pad="60"/>
<connect gate="IO" pin="IO49" pad="61"/>
<connect gate="IO" pin="IO5" pad="7"/>
<connect gate="IO" pin="IO50" pad="63"/>
<connect gate="IO" pin="IO51" pad="64"/>
<connect gate="IO" pin="IO52" pad="65"/>
<connect gate="IO" pin="IO53" pad="67"/>
<connect gate="IO" pin="IO54" pad="68"/>
<connect gate="IO" pin="IO55" pad="69"/>
<connect gate="IO" pin="IO56" pad="70"/>
<connect gate="IO" pin="IO57" pad="71"/>
<connect gate="IO" pin="IO58" pad="72"/>
<connect gate="IO" pin="IO59" pad="75"/>
<connect gate="IO" pin="IO6" pad="8"/>
<connect gate="IO" pin="IO60" pad="76"/>
<connect gate="IO" pin="IO61" pad="77"/>
<connect gate="IO" pin="IO62" pad="78"/>
<connect gate="IO" pin="IO63" pad="79"/>
<connect gate="IO" pin="IO64" pad="80"/>
<connect gate="IO" pin="IO65" pad="81"/>
<connect gate="IO" pin="IO66" pad="83"/>
<connect gate="IO" pin="IO67" pad="84"/>
<connect gate="IO" pin="IO69" pad="92"/>
<connect gate="IO" pin="IO7" pad="9"/>
<connect gate="IO" pin="IO70" pad="93"/>
<connect gate="IO" pin="IO71" pad="94"/>
<connect gate="IO" pin="IO72" pad="96"/>
<connect gate="IO" pin="IO73" pad="97"/>
<connect gate="IO" pin="IO74" pad="98"/>
<connect gate="IO" pin="IO75" pad="99"/>
<connect gate="IO" pin="IO76" pad="100"/>
<connect gate="IO" pin="IO8" pad="10"/>
<connect gate="IO" pin="IO9" pad="12"/>
<connect gate="JEDEC" pin="TCK" pad="62"/>
<connect gate="JEDEC" pin="TDI" pad="4"/>
<connect gate="JEDEC" pin="TDO" pad="73"/>
<connect gate="JEDEC" pin="TMS" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PQFP" package="PQFP-100">
<connects>
<connect gate="G$1" pin="VCCIO" pad="5"/>
<connect gate="G$10" pin="GND" pad="13"/>
<connect gate="G$11" pin="GND" pad="28"/>
<connect gate="G$12" pin="GND" pad="40"/>
<connect gate="G$13" pin="GND" pad="45"/>
<connect gate="G$14" pin="GND" pad="61"/>
<connect gate="G$15" pin="GND" pad="76"/>
<connect gate="G$16" pin="GND" pad="88"/>
<connect gate="G$17" pin="GND" pad="97"/>
<connect gate="G$3" pin="VCCINT" pad="41"/>
<connect gate="G$4" pin="VCCINT" pad="93"/>
<connect gate="G$5" pin="VCCIO" pad="20"/>
<connect gate="G$6" pin="VCCIO" pad="36"/>
<connect gate="G$7" pin="VCCIO" pad="53"/>
<connect gate="G$8" pin="VCCIO" pad="68"/>
<connect gate="G$9" pin="VCCIO" pad="84"/>
<connect gate="IO" pin="IN/GCLK1" pad="89"/>
<connect gate="IO" pin="IN/GCLK2/OE2" pad="92"/>
<connect gate="IO" pin="IN/GCLR" pad="91"/>
<connect gate="IO" pin="IN/OE1" pad="90"/>
<connect gate="IO" pin="IO/GCLK3" pad="87"/>
<connect gate="IO" pin="IO/PD1" pad="3"/>
<connect gate="IO" pin="IO/PD2" pad="43"/>
<connect gate="IO" pin="IO10" pad="15"/>
<connect gate="IO" pin="IO11" pad="16"/>
<connect gate="IO" pin="IO12" pad="18"/>
<connect gate="IO" pin="IO13" pad="19"/>
<connect gate="IO" pin="IO14" pad="21"/>
<connect gate="IO" pin="IO15" pad="22"/>
<connect gate="IO" pin="IO16" pad="23"/>
<connect gate="IO" pin="IO17" pad="24"/>
<connect gate="IO" pin="IO18" pad="25"/>
<connect gate="IO" pin="IO19" pad="26"/>
<connect gate="IO" pin="IO2" pad="4"/>
<connect gate="IO" pin="IO20" pad="27"/>
<connect gate="IO" pin="IO21" pad="29"/>
<connect gate="IO" pin="IO22" pad="30"/>
<connect gate="IO" pin="IO23" pad="31"/>
<connect gate="IO" pin="IO24" pad="32"/>
<connect gate="IO" pin="IO25" pad="33"/>
<connect gate="IO" pin="IO26" pad="34"/>
<connect gate="IO" pin="IO27" pad="35"/>
<connect gate="IO" pin="IO28" pad="37"/>
<connect gate="IO" pin="IO29" pad="38"/>
<connect gate="IO" pin="IO3" pad="7"/>
<connect gate="IO" pin="IO30" pad="39"/>
<connect gate="IO" pin="IO31" pad="42"/>
<connect gate="IO" pin="IO33" pad="44"/>
<connect gate="IO" pin="IO34" pad="46"/>
<connect gate="IO" pin="IO35" pad="47"/>
<connect gate="IO" pin="IO36" pad="48"/>
<connect gate="IO" pin="IO37" pad="49"/>
<connect gate="IO" pin="IO38" pad="50"/>
<connect gate="IO" pin="IO39" pad="51"/>
<connect gate="IO" pin="IO4" pad="8"/>
<connect gate="IO" pin="IO40" pad="52"/>
<connect gate="IO" pin="IO41" pad="54"/>
<connect gate="IO" pin="IO42" pad="55"/>
<connect gate="IO" pin="IO43" pad="56"/>
<connect gate="IO" pin="IO44" pad="57"/>
<connect gate="IO" pin="IO45" pad="58"/>
<connect gate="IO" pin="IO46" pad="59"/>
<connect gate="IO" pin="IO47" pad="60"/>
<connect gate="IO" pin="IO48" pad="62"/>
<connect gate="IO" pin="IO49" pad="63"/>
<connect gate="IO" pin="IO5" pad="9"/>
<connect gate="IO" pin="IO50" pad="65"/>
<connect gate="IO" pin="IO51" pad="66"/>
<connect gate="IO" pin="IO52" pad="67"/>
<connect gate="IO" pin="IO53" pad="69"/>
<connect gate="IO" pin="IO54" pad="70"/>
<connect gate="IO" pin="IO55" pad="71"/>
<connect gate="IO" pin="IO56" pad="72"/>
<connect gate="IO" pin="IO57" pad="73"/>
<connect gate="IO" pin="IO58" pad="74"/>
<connect gate="IO" pin="IO59" pad="77"/>
<connect gate="IO" pin="IO6" pad="10"/>
<connect gate="IO" pin="IO60" pad="78"/>
<connect gate="IO" pin="IO61" pad="79"/>
<connect gate="IO" pin="IO62" pad="80"/>
<connect gate="IO" pin="IO63" pad="81"/>
<connect gate="IO" pin="IO64" pad="82"/>
<connect gate="IO" pin="IO65" pad="83"/>
<connect gate="IO" pin="IO66" pad="85"/>
<connect gate="IO" pin="IO67" pad="86"/>
<connect gate="IO" pin="IO69" pad="94"/>
<connect gate="IO" pin="IO7" pad="11"/>
<connect gate="IO" pin="IO70" pad="95"/>
<connect gate="IO" pin="IO71" pad="96"/>
<connect gate="IO" pin="IO72" pad="98"/>
<connect gate="IO" pin="IO73" pad="99"/>
<connect gate="IO" pin="IO74" pad="100"/>
<connect gate="IO" pin="IO75" pad="1"/>
<connect gate="IO" pin="IO76" pad="2"/>
<connect gate="IO" pin="IO8" pad="12"/>
<connect gate="IO" pin="IO9" pad="14"/>
<connect gate="JEDEC" pin="TCK" pad="64"/>
<connect gate="JEDEC" pin="TDI" pad="6"/>
<connect gate="JEDEC" pin="TDO" pad="75"/>
<connect gate="JEDEC" pin="TMS" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH" package="TH-100">
<connects>
<connect gate="G$1" pin="VCCIO" pad="5"/>
<connect gate="G$10" pin="GND" pad="13"/>
<connect gate="G$11" pin="GND" pad="28"/>
<connect gate="G$12" pin="GND" pad="40"/>
<connect gate="G$13" pin="GND" pad="45"/>
<connect gate="G$14" pin="GND" pad="61"/>
<connect gate="G$15" pin="GND" pad="76"/>
<connect gate="G$16" pin="GND" pad="88"/>
<connect gate="G$17" pin="GND" pad="97"/>
<connect gate="G$3" pin="VCCINT" pad="41"/>
<connect gate="G$4" pin="VCCINT" pad="93"/>
<connect gate="G$5" pin="VCCIO" pad="20"/>
<connect gate="G$6" pin="VCCIO" pad="36"/>
<connect gate="G$7" pin="VCCIO" pad="53"/>
<connect gate="G$8" pin="VCCIO" pad="68"/>
<connect gate="G$9" pin="VCCIO" pad="84"/>
<connect gate="IO" pin="IN/GCLK1" pad="89"/>
<connect gate="IO" pin="IN/GCLK2/OE2" pad="92"/>
<connect gate="IO" pin="IN/GCLR" pad="91"/>
<connect gate="IO" pin="IN/OE1" pad="90"/>
<connect gate="IO" pin="IO/GCLK3" pad="87"/>
<connect gate="IO" pin="IO/PD1" pad="3"/>
<connect gate="IO" pin="IO/PD2" pad="43"/>
<connect gate="IO" pin="IO10" pad="15"/>
<connect gate="IO" pin="IO11" pad="16"/>
<connect gate="IO" pin="IO12" pad="18"/>
<connect gate="IO" pin="IO13" pad="19"/>
<connect gate="IO" pin="IO14" pad="21"/>
<connect gate="IO" pin="IO15" pad="22"/>
<connect gate="IO" pin="IO16" pad="23"/>
<connect gate="IO" pin="IO17" pad="24"/>
<connect gate="IO" pin="IO18" pad="25"/>
<connect gate="IO" pin="IO19" pad="26"/>
<connect gate="IO" pin="IO2" pad="4"/>
<connect gate="IO" pin="IO20" pad="27"/>
<connect gate="IO" pin="IO21" pad="29"/>
<connect gate="IO" pin="IO22" pad="30"/>
<connect gate="IO" pin="IO23" pad="31"/>
<connect gate="IO" pin="IO24" pad="32"/>
<connect gate="IO" pin="IO25" pad="33"/>
<connect gate="IO" pin="IO26" pad="34"/>
<connect gate="IO" pin="IO27" pad="35"/>
<connect gate="IO" pin="IO28" pad="37"/>
<connect gate="IO" pin="IO29" pad="38"/>
<connect gate="IO" pin="IO3" pad="7"/>
<connect gate="IO" pin="IO30" pad="39"/>
<connect gate="IO" pin="IO31" pad="42"/>
<connect gate="IO" pin="IO33" pad="44"/>
<connect gate="IO" pin="IO34" pad="46"/>
<connect gate="IO" pin="IO35" pad="47"/>
<connect gate="IO" pin="IO36" pad="48"/>
<connect gate="IO" pin="IO37" pad="49"/>
<connect gate="IO" pin="IO38" pad="50"/>
<connect gate="IO" pin="IO39" pad="51"/>
<connect gate="IO" pin="IO4" pad="8"/>
<connect gate="IO" pin="IO40" pad="52"/>
<connect gate="IO" pin="IO41" pad="54"/>
<connect gate="IO" pin="IO42" pad="55"/>
<connect gate="IO" pin="IO43" pad="56"/>
<connect gate="IO" pin="IO44" pad="57"/>
<connect gate="IO" pin="IO45" pad="58"/>
<connect gate="IO" pin="IO46" pad="59"/>
<connect gate="IO" pin="IO47" pad="60"/>
<connect gate="IO" pin="IO48" pad="62"/>
<connect gate="IO" pin="IO49" pad="63"/>
<connect gate="IO" pin="IO5" pad="9"/>
<connect gate="IO" pin="IO50" pad="65"/>
<connect gate="IO" pin="IO51" pad="66"/>
<connect gate="IO" pin="IO52" pad="67"/>
<connect gate="IO" pin="IO53" pad="69"/>
<connect gate="IO" pin="IO54" pad="70"/>
<connect gate="IO" pin="IO55" pad="71"/>
<connect gate="IO" pin="IO56" pad="72"/>
<connect gate="IO" pin="IO57" pad="73"/>
<connect gate="IO" pin="IO58" pad="74"/>
<connect gate="IO" pin="IO59" pad="77"/>
<connect gate="IO" pin="IO6" pad="10"/>
<connect gate="IO" pin="IO60" pad="78"/>
<connect gate="IO" pin="IO61" pad="79"/>
<connect gate="IO" pin="IO62" pad="80"/>
<connect gate="IO" pin="IO63" pad="81"/>
<connect gate="IO" pin="IO64" pad="82"/>
<connect gate="IO" pin="IO65" pad="83"/>
<connect gate="IO" pin="IO66" pad="85"/>
<connect gate="IO" pin="IO67" pad="86"/>
<connect gate="IO" pin="IO69" pad="94"/>
<connect gate="IO" pin="IO7" pad="11"/>
<connect gate="IO" pin="IO70" pad="95"/>
<connect gate="IO" pin="IO71" pad="96"/>
<connect gate="IO" pin="IO72" pad="98"/>
<connect gate="IO" pin="IO73" pad="99"/>
<connect gate="IO" pin="IO74" pad="100"/>
<connect gate="IO" pin="IO75" pad="1"/>
<connect gate="IO" pin="IO76" pad="2"/>
<connect gate="IO" pin="IO8" pad="12"/>
<connect gate="IO" pin="IO9" pad="14"/>
<connect gate="JEDEC" pin="TCK" pad="64"/>
<connect gate="JEDEC" pin="TDI" pad="6"/>
<connect gate="JEDEC" pin="TDO" pad="75"/>
<connect gate="JEDEC" pin="TMS" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="X" package="TH100B">
<connects>
<connect gate="G$1" pin="VCCIO" pad="5"/>
<connect gate="G$10" pin="GND" pad="13 P$28"/>
<connect gate="G$11" pin="GND" pad="28"/>
<connect gate="G$12" pin="GND" pad="40"/>
<connect gate="G$13" pin="GND" pad="45 P$24"/>
<connect gate="G$14" pin="GND" pad="61 P$30"/>
<connect gate="G$15" pin="GND" pad="76"/>
<connect gate="G$16" pin="GND" pad="88"/>
<connect gate="G$17" pin="GND" pad="97 P$26"/>
<connect gate="G$3" pin="VCCINT" pad="41 P$23"/>
<connect gate="G$4" pin="VCCINT" pad="93 P$25"/>
<connect gate="G$5" pin="VCCIO" pad="20 P$27"/>
<connect gate="G$6" pin="VCCIO" pad="36 VCCIO@2"/>
<connect gate="G$7" pin="VCCIO" pad="53 VCCIO@1"/>
<connect gate="G$8" pin="VCCIO" pad="68 P$29"/>
<connect gate="G$9" pin="VCCIO" pad="84"/>
<connect gate="IO" pin="IN/GCLK1" pad="89"/>
<connect gate="IO" pin="IN/GCLK2/OE2" pad="92"/>
<connect gate="IO" pin="IN/GCLR" pad="91"/>
<connect gate="IO" pin="IN/OE1" pad="90"/>
<connect gate="IO" pin="IO/GCLK3" pad="87"/>
<connect gate="IO" pin="IO/PD1" pad="3"/>
<connect gate="IO" pin="IO/PD2" pad="43"/>
<connect gate="IO" pin="IO10" pad="15"/>
<connect gate="IO" pin="IO11" pad="16"/>
<connect gate="IO" pin="IO12" pad="18"/>
<connect gate="IO" pin="IO13" pad="19"/>
<connect gate="IO" pin="IO14" pad="21"/>
<connect gate="IO" pin="IO15" pad="22"/>
<connect gate="IO" pin="IO16" pad="23"/>
<connect gate="IO" pin="IO17" pad="24"/>
<connect gate="IO" pin="IO18" pad="25"/>
<connect gate="IO" pin="IO19" pad="26"/>
<connect gate="IO" pin="IO2" pad="4"/>
<connect gate="IO" pin="IO20" pad="27"/>
<connect gate="IO" pin="IO21" pad="29"/>
<connect gate="IO" pin="IO22" pad="30"/>
<connect gate="IO" pin="IO23" pad="31"/>
<connect gate="IO" pin="IO24" pad="32"/>
<connect gate="IO" pin="IO25" pad="33"/>
<connect gate="IO" pin="IO26" pad="34"/>
<connect gate="IO" pin="IO27" pad="35"/>
<connect gate="IO" pin="IO28" pad="37"/>
<connect gate="IO" pin="IO29" pad="38"/>
<connect gate="IO" pin="IO3" pad="7"/>
<connect gate="IO" pin="IO30" pad="39"/>
<connect gate="IO" pin="IO31" pad="42"/>
<connect gate="IO" pin="IO33" pad="44"/>
<connect gate="IO" pin="IO34" pad="46"/>
<connect gate="IO" pin="IO35" pad="47"/>
<connect gate="IO" pin="IO36" pad="48"/>
<connect gate="IO" pin="IO37" pad="49"/>
<connect gate="IO" pin="IO38" pad="50"/>
<connect gate="IO" pin="IO39" pad="51"/>
<connect gate="IO" pin="IO4" pad="8"/>
<connect gate="IO" pin="IO40" pad="52"/>
<connect gate="IO" pin="IO41" pad="54"/>
<connect gate="IO" pin="IO42" pad="55"/>
<connect gate="IO" pin="IO43" pad="56"/>
<connect gate="IO" pin="IO44" pad="57"/>
<connect gate="IO" pin="IO45" pad="58"/>
<connect gate="IO" pin="IO46" pad="59"/>
<connect gate="IO" pin="IO47" pad="60"/>
<connect gate="IO" pin="IO48" pad="62"/>
<connect gate="IO" pin="IO49" pad="63"/>
<connect gate="IO" pin="IO5" pad="9"/>
<connect gate="IO" pin="IO50" pad="65"/>
<connect gate="IO" pin="IO51" pad="66"/>
<connect gate="IO" pin="IO52" pad="67"/>
<connect gate="IO" pin="IO53" pad="69"/>
<connect gate="IO" pin="IO54" pad="70"/>
<connect gate="IO" pin="IO55" pad="71"/>
<connect gate="IO" pin="IO56" pad="72"/>
<connect gate="IO" pin="IO57" pad="73"/>
<connect gate="IO" pin="IO58" pad="74"/>
<connect gate="IO" pin="IO59" pad="77"/>
<connect gate="IO" pin="IO6" pad="10"/>
<connect gate="IO" pin="IO60" pad="78"/>
<connect gate="IO" pin="IO61" pad="79"/>
<connect gate="IO" pin="IO62" pad="80"/>
<connect gate="IO" pin="IO63" pad="81"/>
<connect gate="IO" pin="IO64" pad="82"/>
<connect gate="IO" pin="IO65" pad="83"/>
<connect gate="IO" pin="IO66" pad="85"/>
<connect gate="IO" pin="IO67" pad="86"/>
<connect gate="IO" pin="IO69" pad="94"/>
<connect gate="IO" pin="IO7" pad="11"/>
<connect gate="IO" pin="IO70" pad="95"/>
<connect gate="IO" pin="IO71" pad="96"/>
<connect gate="IO" pin="IO72" pad="98"/>
<connect gate="IO" pin="IO73" pad="99"/>
<connect gate="IO" pin="IO74" pad="100"/>
<connect gate="IO" pin="IO75" pad="1"/>
<connect gate="IO" pin="IO76" pad="2"/>
<connect gate="IO" pin="IO8" pad="12"/>
<connect gate="IO" pin="IO9" pad="14"/>
<connect gate="JEDEC" pin="TCK" pad="64"/>
<connect gate="JEDEC" pin="TDI" pad="6"/>
<connect gate="JEDEC" pin="TDO" pad="75"/>
<connect gate="JEDEC" pin="TMS" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATF150X84" prefix="E">
<description>ATF150x in 84 pin package.</description>
<gates>
<gate name="IO" symbol="AT1508-84"/>
<gate name="JTAG" symbol="JTAG"/>
<gate name="G$1" symbol="PGND"/>
<gate name="G$2" symbol="PGND"/>
<gate name="G$3" symbol="PGND"/>
<gate name="G$4" symbol="PGND"/>
<gate name="G$5" symbol="PGND"/>
<gate name="G$6" symbol="PGND"/>
<gate name="G$7" symbol="PGND"/>
<gate name="G$8" symbol="PGND"/>
<gate name="G$9" symbol="PVCCINT"/>
<gate name="G$10" symbol="PVCCINT"/>
<gate name="G$11" symbol="PVCCIO"/>
<gate name="G$12" symbol="PVCCIO"/>
<gate name="G$13" symbol="PVCCIO"/>
<gate name="G$14" symbol="PVCCIO"/>
<gate name="G$15" symbol="PVCCIO"/>
<gate name="G$16" symbol="PVCCIO"/>
</gates>
<devices>
<device name="" package="S84">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$10" pin="VCCINT" pad="43"/>
<connect gate="G$11" pin="VCCIO" pad="13"/>
<connect gate="G$12" pin="VCCIO" pad="26"/>
<connect gate="G$13" pin="VCCIO" pad="38"/>
<connect gate="G$14" pin="VCCIO" pad="53"/>
<connect gate="G$15" pin="VCCIO" pad="66"/>
<connect gate="G$16" pin="VCCIO" pad="78"/>
<connect gate="G$2" pin="GND" pad="19"/>
<connect gate="G$3" pin="GND" pad="32"/>
<connect gate="G$4" pin="GND" pad="42"/>
<connect gate="G$5" pin="GND" pad="47"/>
<connect gate="G$6" pin="GND" pad="59"/>
<connect gate="G$7" pin="GND" pad="72"/>
<connect gate="G$8" pin="GND" pad="82"/>
<connect gate="G$9" pin="VCCINT" pad="3"/>
<connect gate="IO" pin="IN/GCLK1" pad="83"/>
<connect gate="IO" pin="IN/GCLK2/OE2" pad="2"/>
<connect gate="IO" pin="IN/GCLR" pad="1"/>
<connect gate="IO" pin="IN/OE1" pad="84"/>
<connect gate="IO" pin="IO/GCLK3" pad="81"/>
<connect gate="IO" pin="IO/PD1" pad="12"/>
<connect gate="IO" pin="IO/PD2" pad="45"/>
<connect gate="IO" pin="IO1" pad="4"/>
<connect gate="IO" pin="IO10" pad="16"/>
<connect gate="IO" pin="IO11" pad="17"/>
<connect gate="IO" pin="IO12" pad="18"/>
<connect gate="IO" pin="IO13" pad="20"/>
<connect gate="IO" pin="IO14" pad="21"/>
<connect gate="IO" pin="IO15" pad="22"/>
<connect gate="IO" pin="IO16" pad="24"/>
<connect gate="IO" pin="IO17" pad="25"/>
<connect gate="IO" pin="IO18" pad="27"/>
<connect gate="IO" pin="IO19" pad="28"/>
<connect gate="IO" pin="IO2" pad="5"/>
<connect gate="IO" pin="IO20" pad="29"/>
<connect gate="IO" pin="IO21" pad="30"/>
<connect gate="IO" pin="IO22" pad="31"/>
<connect gate="IO" pin="IO23" pad="33"/>
<connect gate="IO" pin="IO24" pad="34"/>
<connect gate="IO" pin="IO25" pad="35"/>
<connect gate="IO" pin="IO26" pad="36"/>
<connect gate="IO" pin="IO27" pad="37"/>
<connect gate="IO" pin="IO28" pad="39"/>
<connect gate="IO" pin="IO29" pad="40"/>
<connect gate="IO" pin="IO3" pad="6"/>
<connect gate="IO" pin="IO30" pad="41"/>
<connect gate="IO" pin="IO31" pad="44"/>
<connect gate="IO" pin="IO33" pad="46"/>
<connect gate="IO" pin="IO34" pad="48"/>
<connect gate="IO" pin="IO35" pad="49"/>
<connect gate="IO" pin="IO36" pad="50"/>
<connect gate="IO" pin="IO37" pad="51"/>
<connect gate="IO" pin="IO38" pad="52"/>
<connect gate="IO" pin="IO39" pad="54"/>
<connect gate="IO" pin="IO4" pad="8"/>
<connect gate="IO" pin="IO40" pad="55"/>
<connect gate="IO" pin="IO41" pad="56"/>
<connect gate="IO" pin="IO42" pad="57"/>
<connect gate="IO" pin="IO43" pad="58"/>
<connect gate="IO" pin="IO44" pad="60"/>
<connect gate="IO" pin="IO45" pad="61"/>
<connect gate="IO" pin="IO46" pad="63"/>
<connect gate="IO" pin="IO47" pad="64"/>
<connect gate="IO" pin="IO48" pad="65"/>
<connect gate="IO" pin="IO49" pad="67"/>
<connect gate="IO" pin="IO5" pad="9"/>
<connect gate="IO" pin="IO50" pad="68"/>
<connect gate="IO" pin="IO51" pad="69"/>
<connect gate="IO" pin="IO52" pad="70"/>
<connect gate="IO" pin="IO53" pad="73"/>
<connect gate="IO" pin="IO54" pad="74"/>
<connect gate="IO" pin="IO55" pad="75"/>
<connect gate="IO" pin="IO56" pad="76"/>
<connect gate="IO" pin="IO57" pad="77"/>
<connect gate="IO" pin="IO58" pad="79"/>
<connect gate="IO" pin="IO59" pad="80"/>
<connect gate="IO" pin="IO6" pad="10"/>
<connect gate="IO" pin="IO7" pad="11"/>
<connect gate="IO" pin="IO9" pad="15"/>
<connect gate="JTAG" pin="TCK" pad="62"/>
<connect gate="JTAG" pin="TDI" pad="14"/>
<connect gate="JTAG" pin="TDO" pad="71"/>
<connect gate="JTAG" pin="TMS" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATF150X44" prefix="E">
<description>ATF150x in 44 pin packages</description>
<gates>
<gate name="A" symbol="AT1504-44"/>
<gate name="G$5" symbol="PGND"/>
<gate name="G$6" symbol="PGND"/>
<gate name="G$7" symbol="PGND"/>
<gate name="G$8" symbol="PGND"/>
<gate name="G$1" symbol="PVCC"/>
<gate name="G$2" symbol="PVCC"/>
<gate name="G$3" symbol="PVCC"/>
<gate name="G$4" symbol="PVCC"/>
</gates>
<devices>
<device name="" package="3M44">
<connects>
<connect gate="A" pin="IN/GCLK1" pad="43"/>
<connect gate="A" pin="IN/GCLR" pad="1"/>
<connect gate="A" pin="IN/OE1" pad="44"/>
<connect gate="A" pin="IN/OE2/GCLK2" pad="2"/>
<connect gate="A" pin="IO1/TDI" pad="7"/>
<connect gate="A" pin="IO10" pad="14"/>
<connect gate="A" pin="IO11" pad="16"/>
<connect gate="A" pin="IO12" pad="17"/>
<connect gate="A" pin="IO13" pad="18"/>
<connect gate="A" pin="IO14" pad="19"/>
<connect gate="A" pin="IO15/PD2" pad="25"/>
<connect gate="A" pin="IO16" pad="20"/>
<connect gate="A" pin="IO17" pad="21"/>
<connect gate="A" pin="IO18" pad="24"/>
<connect gate="A" pin="IO19" pad="26"/>
<connect gate="A" pin="IO2" pad="4"/>
<connect gate="A" pin="IO20" pad="27"/>
<connect gate="A" pin="IO21/TCK" pad="32"/>
<connect gate="A" pin="IO22" pad="28"/>
<connect gate="A" pin="IO23" pad="29"/>
<connect gate="A" pin="IO24" pad="31"/>
<connect gate="A" pin="IO25" pad="33"/>
<connect gate="A" pin="IO26/TDO" pad="38"/>
<connect gate="A" pin="IO27" pad="34"/>
<connect gate="A" pin="IO28" pad="36"/>
<connect gate="A" pin="IO29/GCLK3" pad="41"/>
<connect gate="A" pin="IO3" pad="5"/>
<connect gate="A" pin="IO30" pad="37"/>
<connect gate="A" pin="IO31" pad="39"/>
<connect gate="A" pin="IO32" pad="40"/>
<connect gate="A" pin="IO4/PD1" pad="11"/>
<connect gate="A" pin="IO5" pad="6"/>
<connect gate="A" pin="IO6/TMS" pad="13"/>
<connect gate="A" pin="IO7" pad="8"/>
<connect gate="A" pin="IO8" pad="9"/>
<connect gate="A" pin="IO9" pad="12"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$2" pin="VCC" pad="15"/>
<connect gate="G$3" pin="VCC" pad="23"/>
<connect gate="G$4" pin="VCC" pad="35"/>
<connect gate="G$5" pin="GND" pad="10"/>
<connect gate="G$6" pin="GND" pad="22"/>
<connect gate="G$7" pin="GND" pad="30"/>
<connect gate="G$8" pin="GND" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQFP" package="TQFP44">
<connects>
<connect gate="A" pin="IN/GCLK1" pad="37"/>
<connect gate="A" pin="IN/GCLR" pad="39"/>
<connect gate="A" pin="IN/OE1" pad="38"/>
<connect gate="A" pin="IN/OE2/GCLK2" pad="40"/>
<connect gate="A" pin="IO1/TDI" pad="1"/>
<connect gate="A" pin="IO10" pad="12"/>
<connect gate="A" pin="IO11" pad="13"/>
<connect gate="A" pin="IO12" pad="14"/>
<connect gate="A" pin="IO13" pad="15"/>
<connect gate="A" pin="IO14" pad="18"/>
<connect gate="A" pin="IO15/PD2" pad="19"/>
<connect gate="A" pin="IO16" pad="20"/>
<connect gate="A" pin="IO17" pad="21"/>
<connect gate="A" pin="IO18" pad="22"/>
<connect gate="A" pin="IO19" pad="23"/>
<connect gate="A" pin="IO2" pad="2"/>
<connect gate="A" pin="IO20" pad="25"/>
<connect gate="A" pin="IO21/TCK" pad="26"/>
<connect gate="A" pin="IO22" pad="27"/>
<connect gate="A" pin="IO23" pad="28"/>
<connect gate="A" pin="IO24" pad="30"/>
<connect gate="A" pin="IO25" pad="31"/>
<connect gate="A" pin="IO26/TDO" pad="32"/>
<connect gate="A" pin="IO27" pad="33"/>
<connect gate="A" pin="IO28" pad="34"/>
<connect gate="A" pin="IO29/GCLK3" pad="35"/>
<connect gate="A" pin="IO3" pad="3"/>
<connect gate="A" pin="IO30" pad="42"/>
<connect gate="A" pin="IO31" pad="43"/>
<connect gate="A" pin="IO32" pad="44"/>
<connect gate="A" pin="IO4/PD1" pad="5"/>
<connect gate="A" pin="IO5" pad="6"/>
<connect gate="A" pin="IO6/TMS" pad="7"/>
<connect gate="A" pin="IO7" pad="8"/>
<connect gate="A" pin="IO8" pad="10"/>
<connect gate="A" pin="IO9" pad="11"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$2" pin="VCC" pad="17"/>
<connect gate="G$3" pin="VCC" pad="29"/>
<connect gate="G$4" pin="VCC" pad="41"/>
<connect gate="G$5" pin="GND" pad="4"/>
<connect gate="G$6" pin="GND" pad="16"/>
<connect gate="G$7" pin="GND" pad="24"/>
<connect gate="G$8" pin="GND" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
