<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>//wsl$/Debian/home/vrs/Eagle/projects/DEC/DMM-8E/DMM-8E-2front.bmp</text>
<text>DMM</text>
<text>8E</text>
<text>2</text>
<text>X</text>
<text>MEMORY</text>
<text>MANAGEMENT</text>
<text>COPYRIGHT</text>
<text>DIGICOS</text>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOCKET-16">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO5">
<description>&lt;b&gt;TO 5&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="U$2" library="dec-con" package="EDGE-CON8" value="QUAD"/>
<element name="J1" library="ic-package" package="SOCKET-16" value=" "/>
<element name="E33" library="74xx-us" package="DIL16" value="74LS257N"/>
<element name="E30" library="dec-con" package="DIL14" value="SP314N"/>
<element name="E29" library="dec-con" package="DIL14" value="SP314N"/>
<element name="E20" library="74xx-us" package="DIL16" value="74LS257N"/>
<element name="E23" library="74xx-us" package="DIL16" value="74LS257N"/>
<element name="E27" library="74xx-us" package="DIL16" value="74175N"/>
<element name="E32" library="74xx-us" package="DIL16" value="74175N"/>
<element name="E14" library="74xx-us" package="DIL16" value="74175N"/>
<element name="E8" library="74xx-us" package="DIL16" value="74175N"/>
<element name="E2" library="74xx-us" package="DIL16" value="74175N"/>
<element name="E24" library="74xx-us" package="DIL14" value="7410N"/>
<element name="E5" library="dec-con" package="DIL14" value="SP314N"/>
<element name="E21" library="74xx-us" package="DIL14" value="7408N"/>
<element name="E12" library="74xx-us" package="DIL14" value="7404N"/>
<element name="E6" library="74xx-us" package="DIL14" value="7474N"/>
<element name="E3" library="74xx-us" package="DIL14" value="7474N"/>
<element name="E11" library="74xx-us" package="DIL14" value="7400N"/>
<element name="E28" library="dec-con" package="DIL14" value="SP380N"/>
<element name="E25" library="dec-con" package="DIL14" value="SP380N"/>
<element name="E16" library="dec-con" package="DIL14" value="SP380N"/>
<element name="E10" library="dec-con" package="DIL14" value="SP380N"/>
<element name="E18" library="74xx-us" package="DIL16" value="74155N"/>
<element name="E17" library="74xx-us" package="DIL16" value="74155N"/>
<element name="E9" library="dec-con" package="DIL14" value="74H40N"/>
<element name="E31" library="dec-con" package="DIL16" value="DS8641N"/>
<element name="E13" library="dec-con" package="DIL16" value="DS8641N"/>
<element name="E7" library="dec-con" package="DIL16" value="DS8641N"/>
<element name="E22" library="74xx-us" package="DIL14" value="7401N"/>
<element name="E19" library="74xx-us" package="DIL14" value="7401N"/>
<element name="E1" library="74xx-us" package="DIL14" value="7401N"/>
<element name="E4" library="dec-con" package="DIL14" value="SP380N"/>
<element name="E15" library="74xx-us" package="DIL14" value="7404N"/>
<element name="C1" library="rcl" package="E15-5" value="10uF"/>
<element name="E34" library="dec-con" package="DIL40" value="AM2901"/>
<element name="C2" library="rcl" package="E15-5" value="10uF"/>
<element name="C3" library="rcl" package="E15-5" value="10uF"/>
<element name="C4" library="rcl" package="E15-5" value="10uF"/>
<element name="C5" library="rcl" package="E15-5" value="10uF"/>
<element name="C6" library="rcl" package="E15-5" value="10uF"/>
<element name="C7" library="rcl" package="E15-5" value="10uF"/>
<element name="C8" library="rcl" package="E15-5" value="10uF"/>
<element name="R1" library="rcl" package="0207/10" value="2.2K"/>
<element name="R2" library="rcl" package="0207/10" value="680"/>
<element name="R3" library="rcl" package="0207/10" value="220"/>
<element name="C9" library="rcl" package="B45181C" value="820pF"/>
<element name="R4" library="rcl" package="0207/10" value="220"/>
<element name="C10" library="rcl" package="B45181C" value="820pF"/>
<element name="R5" library="rcl" package="0207/10" value="220"/>
<element name="C11" library="rcl" package="B45181C" value="820pF"/>
<element name="R6" library="rcl" package="0207/10" value="220"/>
<element name="R7" library="rcl" package="0207/10" value="10"/>
<element name="R8" library="rcl" package="0207/10" value="2400"/>
<element name="R9" library="rcl" package="0207/10" value="470"/>
<element name="C12" library="rcl" package="TT5D7" value="15uF"/>
<element name="C13" library="rcl" package="TT5D7" value="15uF"/>
<element name="C14" library="rcl" package="TT5D7" value="15uF"/>
<element name="R10" library="rcl" package="0207/10" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP1" value=" "/>
<element name="E26" library="dec-con" package="DIL16" value="I3107"/>
<element name="Q1" library="transistor" package="TO5" value="OPEN"/>
</elements>
<signals>
<signal name="GND">
<contactref element="E33" pad="8"/>
<contactref element="E30" pad="1"/>
<contactref element="E29" pad="1"/>
<contactref element="E20" pad="8"/>
<contactref element="E23" pad="8"/>
<contactref element="E27" pad="8"/>
<contactref element="E32" pad="8"/>
<contactref element="E14" pad="8"/>
<contactref element="E8" pad="8"/>
<contactref element="E2" pad="8"/>
<contactref element="E24" pad="7"/>
<contactref element="E5" pad="1"/>
<contactref element="E21" pad="7"/>
<contactref element="E12" pad="7"/>
<contactref element="E6" pad="7"/>
<contactref element="E3" pad="7"/>
<contactref element="E11" pad="7"/>
<contactref element="E28" pad="1"/>
<contactref element="E25" pad="1"/>
<contactref element="E16" pad="1"/>
<contactref element="E10" pad="1"/>
<contactref element="E18" pad="8"/>
<contactref element="E17" pad="8"/>
<contactref element="E9" pad="7"/>
<contactref element="E31" pad="8"/>
<contactref element="E13" pad="8"/>
<contactref element="E7" pad="8"/>
<contactref element="E22" pad="7"/>
<contactref element="E19" pad="7"/>
<contactref element="E1" pad="7"/>
<contactref element="E4" pad="1"/>
<contactref element="E15" pad="7"/>
<contactref element="U$2" pad="AC1"/>
<contactref element="U$2" pad="AF1"/>
<contactref element="U$2" pad="AN1"/>
<contactref element="U$2" pad="AT1"/>
<contactref element="U$2" pad="BC1"/>
<contactref element="U$2" pad="BF1"/>
<contactref element="U$2" pad="BN1"/>
<contactref element="U$2" pad="BT1"/>
<contactref element="U$2" pad="CT1"/>
<contactref element="U$2" pad="CN1"/>
<contactref element="U$2" pad="AC2"/>
<contactref element="U$2" pad="AF2"/>
<contactref element="U$2" pad="AN2"/>
<contactref element="U$2" pad="AT2"/>
<contactref element="U$2" pad="BC2"/>
<contactref element="U$2" pad="BF2"/>
<contactref element="U$2" pad="BN2"/>
<contactref element="U$2" pad="CC2"/>
<contactref element="U$2" pad="CN2"/>
<contactref element="U$2" pad="CT2"/>
<contactref element="U$2" pad="DC2"/>
<contactref element="U$2" pad="DF2"/>
<contactref element="U$2" pad="DF1"/>
<contactref element="U$2" pad="DC1"/>
<contactref element="U$2" pad="DT2"/>
<contactref element="U$2" pad="DT1"/>
<contactref element="U$2" pad="BT2"/>
<contactref element="U$2" pad="CC1"/>
<contactref element="C1" pad="-"/>
<contactref element="E34" pad="30"/>
<contactref element="E34" pad="26"/>
<contactref element="C8" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="C7" pad="-"/>
<contactref element="E28" pad="10"/>
<contactref element="E28" pad="11"/>
<contactref element="E28" pad="5"/>
<contactref element="E28" pad="6"/>
<contactref element="E25" pad="6"/>
<contactref element="E25" pad="5"/>
<contactref element="E25" pad="10"/>
<contactref element="E34" pad="22"/>
<contactref element="E34" pad="40"/>
<contactref element="E34" pad="20"/>
<contactref element="E34" pad="1"/>
<contactref element="E34" pad="12"/>
<contactref element="E34" pad="5"/>
<contactref element="E34" pad="6"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="9"/>
<contactref element="C9" pad="-"/>
<contactref element="E4" pad="10"/>
<contactref element="E4" pad="11"/>
<contactref element="E10" pad="6"/>
<contactref element="E10" pad="5"/>
<contactref element="E10" pad="11"/>
<contactref element="E10" pad="10"/>
<contactref element="E16" pad="6"/>
<contactref element="E16" pad="5"/>
<contactref element="E16" pad="10"/>
<contactref element="E4" pad="5"/>
<contactref element="E4" pad="6"/>
<contactref element="C10" pad="-"/>
<contactref element="C11" pad="-"/>
<contactref element="C12" pad="-"/>
<contactref element="C14" pad="-"/>
<contactref element="C13" pad="-"/>
<contactref element="R9" pad="2"/>
<contactref element="E34" pad="29"/>
<contactref element="E34" pad="31"/>
<contactref element="E26" pad="8"/>
<contactref element="E33" pad="15"/>
<contactref element="E23" pad="15"/>
<contactref element="E20" pad="15"/>
<contactref element="E26" pad="2"/>
<contactref element="E26" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="E33" pad="16"/>
<contactref element="E30" pad="8"/>
<contactref element="E29" pad="8"/>
<contactref element="E20" pad="16"/>
<contactref element="E23" pad="16"/>
<contactref element="E27" pad="16"/>
<contactref element="E32" pad="16"/>
<contactref element="E14" pad="16"/>
<contactref element="E8" pad="16"/>
<contactref element="E2" pad="16"/>
<contactref element="E24" pad="14"/>
<contactref element="E5" pad="8"/>
<contactref element="E21" pad="14"/>
<contactref element="E12" pad="14"/>
<contactref element="E6" pad="14"/>
<contactref element="E3" pad="14"/>
<contactref element="E11" pad="14"/>
<contactref element="E28" pad="8"/>
<contactref element="E25" pad="8"/>
<contactref element="E16" pad="8"/>
<contactref element="E10" pad="8"/>
<contactref element="E18" pad="16"/>
<contactref element="E17" pad="16"/>
<contactref element="E9" pad="14"/>
<contactref element="E31" pad="16"/>
<contactref element="E13" pad="16"/>
<contactref element="E7" pad="16"/>
<contactref element="E22" pad="14"/>
<contactref element="E19" pad="14"/>
<contactref element="E1" pad="14"/>
<contactref element="E4" pad="8"/>
<contactref element="E15" pad="14"/>
<contactref element="U$2" pad="AA2"/>
<contactref element="U$2" pad="BA2"/>
<contactref element="U$2" pad="CA2"/>
<contactref element="C1" pad="+"/>
<contactref element="E34" pad="10"/>
<contactref element="E34" pad="28"/>
<contactref element="C8" pad="+"/>
<contactref element="C2" pad="+"/>
<contactref element="C3" pad="+"/>
<contactref element="C4" pad="+"/>
<contactref element="C5" pad="+"/>
<contactref element="C6" pad="+"/>
<contactref element="C7" pad="+"/>
<contactref element="E34" pad="7"/>
<contactref element="E34" pad="14"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="C12" pad="+"/>
<contactref element="C13" pad="+"/>
<contactref element="C14" pad="+"/>
<contactref element="R10" pad="1"/>
<contactref element="E34" pad="27"/>
<contactref element="E26" pad="16"/>
<contactref element="E6" pad="10"/>
<contactref element="E6" pad="4"/>
<contactref element="E14" pad="1"/>
<contactref element="E32" pad="1"/>
</signal>
<signal name="!DATA03">
<contactref element="U$2" pad="AV1"/>
<contactref element="E7" pad="4"/>
</signal>
<signal name="!MD00">
<contactref element="U$2" pad="AK1"/>
<contactref element="E5" pad="10"/>
<contactref element="E4" pad="9"/>
</signal>
<signal name="!MD01">
<contactref element="U$2" pad="AL1"/>
<contactref element="E5" pad="9"/>
<contactref element="E4" pad="12"/>
</signal>
<signal name="!MD02">
<contactref element="U$2" pad="AM1"/>
<contactref element="E4" pad="4"/>
</signal>
<signal name="!MD03">
<contactref element="U$2" pad="AP1"/>
<contactref element="E4" pad="7"/>
</signal>
<signal name="!DATA00">
<contactref element="U$2" pad="AR1"/>
<contactref element="E7" pad="12"/>
</signal>
<signal name="!DATA01">
<contactref element="U$2" pad="AS1"/>
<contactref element="E7" pad="15"/>
</signal>
<signal name="!DATA02">
<contactref element="U$2" pad="AU1"/>
<contactref element="E7" pad="1"/>
</signal>
<signal name="!EMA2">
<contactref element="U$2" pad="AH2"/>
<contactref element="E1" pad="4"/>
</signal>
<signal name="!EMA1">
<contactref element="U$2" pad="AE2"/>
<contactref element="E1" pad="1"/>
</signal>
<signal name="!EMA0">
<contactref element="U$2" pad="AD2"/>
<contactref element="E1" pad="13"/>
</signal>
<signal name="LOAD_CNTL">
<contactref element="U$2" pad="BH2"/>
<contactref element="E16" pad="9"/>
</signal>
<signal name="!TS2">
<contactref element="U$2" pad="CL2"/>
<contactref element="E6" pad="3"/>
</signal>
<signal name="TP4">
<contactref element="U$2" pad="CJ2"/>
<contactref element="E25" pad="9"/>
</signal>
<signal name="TP3">
<contactref element="U$2" pad="CH2"/>
<contactref element="E16" pad="4"/>
</signal>
<signal name="TP2">
<contactref element="U$2" pad="CE2"/>
</signal>
<signal name="!DATA07">
<contactref element="U$2" pad="BV1"/>
<contactref element="E13" pad="4"/>
</signal>
<signal name="!DATA06">
<contactref element="U$2" pad="BU1"/>
<contactref element="E13" pad="1"/>
</signal>
<signal name="!DATA05">
<contactref element="U$2" pad="BS1"/>
<contactref element="E13" pad="15"/>
</signal>
<signal name="!DATA04">
<contactref element="U$2" pad="BR1"/>
<contactref element="E13" pad="12"/>
</signal>
<signal name="!MD07">
<contactref element="U$2" pad="BP1"/>
<contactref element="E10" pad="7"/>
</signal>
<signal name="!MD06">
<contactref element="U$2" pad="BM1"/>
<contactref element="E10" pad="4"/>
</signal>
<signal name="!MD05">
<contactref element="U$2" pad="BL1"/>
<contactref element="E10" pad="12"/>
</signal>
<signal name="!MD04">
<contactref element="U$2" pad="BK1"/>
<contactref element="E10" pad="9"/>
<contactref element="E30" pad="10"/>
<contactref element="E29" pad="11"/>
</signal>
<signal name="!CPMA_DISABLE">
<contactref element="U$2" pad="CU1"/>
<contactref element="E25" pad="4"/>
</signal>
<signal name="!SKIP">
<contactref element="U$2" pad="CS1"/>
<contactref element="E22" pad="4"/>
</signal>
<signal name="!NOT_LAST_XFR">
<contactref element="U$2" pad="CM1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="!INTERNAL_IO">
<contactref element="U$2" pad="CL1"/>
<contactref element="E16" pad="7"/>
<contactref element="E22" pad="13"/>
<contactref element="E22" pad="10"/>
</signal>
<signal name="!C1">
<contactref element="U$2" pad="CH1"/>
<contactref element="E19" pad="1"/>
</signal>
<signal name="!C0">
<contactref element="U$2" pad="CE1"/>
<contactref element="E19" pad="4"/>
<contactref element="E19" pad="13"/>
<contactref element="E19" pad="10"/>
</signal>
<signal name="!IO_PAUSE">
<contactref element="U$2" pad="CD1"/>
<contactref element="E29" pad="12"/>
</signal>
<signal name="!F_SET">
<contactref element="U$2" pad="DR2"/>
<contactref element="E25" pad="7"/>
</signal>
<signal name="!USER_MODE">
<contactref element="U$2" pad="DM2"/>
<contactref element="E9" pad="8"/>
</signal>
<signal name="!F">
<contactref element="U$2" pad="DJ2"/>
<contactref element="E5" pad="4"/>
</signal>
<signal name="!DATA11">
<contactref element="U$2" pad="DV1"/>
<contactref element="E31" pad="4"/>
</signal>
<signal name="!DATA10">
<contactref element="U$2" pad="DU1"/>
<contactref element="E31" pad="1"/>
</signal>
<signal name="!DATA09">
<contactref element="U$2" pad="DS1"/>
<contactref element="E31" pad="15"/>
</signal>
<signal name="!DATA08">
<contactref element="U$2" pad="DR1"/>
<contactref element="E31" pad="12"/>
</signal>
<signal name="!MD11">
<contactref element="U$2" pad="DP1"/>
<contactref element="E28" pad="7"/>
<contactref element="E29" pad="6"/>
</signal>
<signal name="!MD10">
<contactref element="U$2" pad="DM1"/>
<contactref element="E28" pad="4"/>
</signal>
<signal name="!MD09">
<contactref element="U$2" pad="DL1"/>
<contactref element="E28" pad="12"/>
<contactref element="E30" pad="6"/>
<contactref element="E29" pad="4"/>
</signal>
<signal name="!MD08">
<contactref element="U$2" pad="DK1"/>
<contactref element="E28" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="E34" pad="36"/>
<contactref element="E2" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="E34" pad="37"/>
<contactref element="E2" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="E34" pad="38"/>
<contactref element="E2" pad="12"/>
</signal>
<signal name="DATA08">
<contactref element="E34" pad="25"/>
<contactref element="E31" pad="10"/>
<contactref element="E23" pad="6"/>
</signal>
<signal name="DATA07">
<contactref element="E34" pad="24"/>
<contactref element="E13" pad="6"/>
<contactref element="E23" pad="10"/>
</signal>
<signal name="DATA06">
<contactref element="E34" pad="23"/>
<contactref element="E13" pad="3"/>
<contactref element="E23" pad="13"/>
</signal>
<signal name="DATA11">
<contactref element="E34" pad="17"/>
<contactref element="E31" pad="6"/>
<contactref element="E26" pad="13"/>
</signal>
<signal name="DATA10">
<contactref element="E34" pad="18"/>
<contactref element="E31" pad="3"/>
</signal>
<signal name="DATA09">
<contactref element="E34" pad="19"/>
<contactref element="E31" pad="13"/>
</signal>
<signal name="N$10">
<contactref element="E1" pad="8"/>
<contactref element="R3" pad="1"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$11">
<contactref element="E1" pad="9"/>
<contactref element="E6" pad="5"/>
<contactref element="E9" pad="5"/>
<contactref element="E9" pad="1"/>
<contactref element="E9" pad="2"/>
<contactref element="E9" pad="4"/>
</signal>
<signal name="MD09">
<contactref element="E32" pad="12"/>
<contactref element="E28" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="E1" pad="10"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="DATA04">
<contactref element="E13" pad="10"/>
<contactref element="E20" pad="10"/>
</signal>
<signal name="DATA03">
<contactref element="E7" pad="6"/>
<contactref element="E20" pad="13"/>
</signal>
<signal name="!RTM">
<contactref element="E31" pad="9"/>
<contactref element="E31" pad="7"/>
<contactref element="E7" pad="7"/>
<contactref element="E7" pad="9"/>
<contactref element="E13" pad="7"/>
<contactref element="E13" pad="9"/>
<contactref element="E17" pad="9"/>
<contactref element="E15" pad="13"/>
</signal>
<signal name="MME">
<contactref element="E22" pad="6"/>
<contactref element="E3" pad="5"/>
<contactref element="E11" pad="9"/>
</signal>
<signal name="LTM">
<contactref element="E22" pad="3"/>
<contactref element="E22" pad="2"/>
<contactref element="E11" pad="1"/>
<contactref element="E15" pad="2"/>
<contactref element="E19" pad="12"/>
<contactref element="E19" pad="11"/>
<contactref element="E20" pad="1"/>
<contactref element="E23" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="!LOAD_CNTL">
<contactref element="E16" pad="14"/>
<contactref element="E25" pad="11"/>
<contactref element="E16" pad="12"/>
<contactref element="E16" pad="11"/>
</signal>
<signal name="N$20">
<contactref element="E23" pad="12"/>
<contactref element="E26" pad="9"/>
</signal>
<signal name="MD07">
<contactref element="E10" pad="2"/>
<contactref element="E18" pad="3"/>
<contactref element="E17" pad="3"/>
<contactref element="E14" pad="4"/>
<contactref element="E23" pad="11"/>
</signal>
<signal name="N$22">
<contactref element="E27" pad="10"/>
<contactref element="E2" pad="13"/>
<contactref element="E11" pad="10"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="BLOAD_CNTL">
<contactref element="E16" pad="13"/>
<contactref element="E21" pad="2"/>
</signal>
<signal name="!CMME">
<contactref element="E11" pad="4"/>
<contactref element="E3" pad="2"/>
<contactref element="E17" pad="4"/>
</signal>
<signal name="!SMME">
<contactref element="E11" pad="5"/>
<contactref element="E17" pad="5"/>
</signal>
<signal name="MD06">
<contactref element="E10" pad="3"/>
<contactref element="E14" pad="5"/>
<contactref element="E17" pad="15"/>
<contactref element="E23" pad="14"/>
<contactref element="E18" pad="1"/>
<contactref element="E17" pad="1"/>
<contactref element="E18" pad="15"/>
</signal>
<signal name="MD08">
<contactref element="E32" pad="13"/>
<contactref element="E17" pad="13"/>
<contactref element="E28" pad="14"/>
<contactref element="E23" pad="5"/>
<contactref element="E18" pad="13"/>
</signal>
<signal name="MD03">
<contactref element="E8" pad="4"/>
<contactref element="E20" pad="14"/>
<contactref element="E29" pad="9"/>
<contactref element="E30" pad="12"/>
<contactref element="E4" pad="2"/>
</signal>
<signal name="MD05">
<contactref element="E10" pad="13"/>
<contactref element="E14" pad="12"/>
<contactref element="E20" pad="5"/>
<contactref element="E30" pad="11"/>
<contactref element="E29" pad="10"/>
</signal>
<signal name="MD02">
<contactref element="E5" pad="6"/>
<contactref element="E8" pad="5"/>
<contactref element="E4" pad="3"/>
<contactref element="E5" pad="5"/>
<contactref element="E5" pad="11"/>
<contactref element="E5" pad="12"/>
</signal>
<signal name="MD01">
<contactref element="E4" pad="13"/>
<contactref element="E8" pad="12"/>
</signal>
<signal name="MD11">
<contactref element="E28" pad="2"/>
<contactref element="E32" pad="4"/>
</signal>
<signal name="MD10">
<contactref element="E28" pad="3"/>
<contactref element="E30" pad="5"/>
<contactref element="E29" pad="5"/>
<contactref element="E32" pad="5"/>
</signal>
<signal name="TRAP">
<contactref element="J1" pad="7"/>
<contactref element="E32" pad="9"/>
<contactref element="E8" pad="9"/>
<contactref element="E14" pad="9"/>
</signal>
<signal name="MD00">
<contactref element="E4" pad="14"/>
<contactref element="E8" pad="13"/>
</signal>
<signal name="N$42">
<contactref element="E2" pad="15"/>
<contactref element="E9" pad="9"/>
<contactref element="E9" pad="10"/>
</signal>
<signal name="!LTM">
<contactref element="R5" pad="2"/>
<contactref element="E17" pad="12"/>
<contactref element="E15" pad="1"/>
</signal>
<signal name="!LRM">
<contactref element="R4" pad="2"/>
<contactref element="E15" pad="11"/>
<contactref element="E17" pad="7"/>
</signal>
<signal name="N$45">
<contactref element="E21" pad="8"/>
<contactref element="E26" pad="5"/>
<contactref element="E26" pad="4"/>
<contactref element="E26" pad="3"/>
</signal>
<signal name="!IFDF_CLR">
<contactref element="J1" pad="3"/>
<contactref element="E21" pad="12"/>
</signal>
<signal name="IOT2X_45">
<contactref element="E12" pad="1"/>
<contactref element="E24" pad="11"/>
<contactref element="E30" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="E30" pad="9"/>
<contactref element="E12" pad="6"/>
</signal>
<signal name="N$51">
<contactref element="E33" pad="1"/>
<contactref element="E6" pad="9"/>
</signal>
<signal name="N$52">
<contactref element="E34" pad="15"/>
<contactref element="E11" pad="11"/>
</signal>
<signal name="LRM">
<contactref element="E34" pad="13"/>
<contactref element="E11" pad="13"/>
<contactref element="E15" pad="10"/>
<contactref element="E19" pad="9"/>
<contactref element="E19" pad="8"/>
</signal>
<signal name="N$54">
<contactref element="E34" pad="4"/>
<contactref element="E33" pad="7"/>
</signal>
<signal name="N$55">
<contactref element="E34" pad="3"/>
<contactref element="E33" pad="4"/>
</signal>
<signal name="N$56">
<contactref element="E34" pad="2"/>
<contactref element="E33" pad="12"/>
</signal>
<signal name="IOT2X5">
<contactref element="E12" pad="3"/>
<contactref element="E29" pad="3"/>
<contactref element="E22" pad="9"/>
<contactref element="E22" pad="8"/>
</signal>
<signal name="!TP4">
<contactref element="E12" pad="9"/>
<contactref element="E25" pad="12"/>
<contactref element="E25" pad="14"/>
</signal>
<signal name="N$59">
<contactref element="E3" pad="10"/>
<contactref element="E2" pad="1"/>
<contactref element="E21" pad="11"/>
<contactref element="E27" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="E3" pad="8"/>
<contactref element="E1" pad="6"/>
<contactref element="E1" pad="3"/>
<contactref element="E1" pad="11"/>
</signal>
<signal name="N$72">
<contactref element="E1" pad="5"/>
<contactref element="E2" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="E1" pad="2"/>
<contactref element="E2" pad="7"/>
</signal>
<signal name="N$74">
<contactref element="E1" pad="12"/>
<contactref element="E2" pad="10"/>
</signal>
<signal name="N$77">
<contactref element="E31" pad="11"/>
<contactref element="E32" pad="15"/>
</signal>
<signal name="N$78">
<contactref element="E31" pad="14"/>
<contactref element="E32" pad="10"/>
</signal>
<signal name="N$80">
<contactref element="E31" pad="5"/>
<contactref element="E32" pad="2"/>
</signal>
<signal name="N$81">
<contactref element="E31" pad="2"/>
<contactref element="E32" pad="7"/>
</signal>
<signal name="N$83">
<contactref element="E13" pad="11"/>
<contactref element="E14" pad="15"/>
</signal>
<signal name="N$84">
<contactref element="E13" pad="14"/>
<contactref element="E14" pad="10"/>
</signal>
<signal name="N$86">
<contactref element="E13" pad="5"/>
<contactref element="E14" pad="2"/>
</signal>
<signal name="N$87">
<contactref element="E13" pad="2"/>
<contactref element="E14" pad="7"/>
</signal>
<signal name="DATA05">
<contactref element="E13" pad="13"/>
<contactref element="E20" pad="6"/>
</signal>
<signal name="N$89">
<contactref element="E7" pad="11"/>
<contactref element="E8" pad="15"/>
</signal>
<signal name="N$90">
<contactref element="E7" pad="14"/>
<contactref element="E8" pad="10"/>
</signal>
<signal name="N$92">
<contactref element="E7" pad="5"/>
<contactref element="E8" pad="2"/>
</signal>
<signal name="N$93">
<contactref element="E7" pad="2"/>
<contactref element="E8" pad="7"/>
</signal>
<signal name="DATA01">
<contactref element="E7" pad="13"/>
</signal>
<signal name="DATA02">
<contactref element="E7" pad="3"/>
</signal>
<signal name="DATA00">
<contactref element="E7" pad="10"/>
</signal>
<signal name="N$143">
<contactref element="E33" pad="2"/>
<contactref element="E27" pad="2"/>
</signal>
<signal name="DF1_IN">
<contactref element="E33" pad="3"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="DF2_IN">
<contactref element="E33" pad="6"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="DF0_IN">
<contactref element="J1" pad="12"/>
<contactref element="E33" pad="13"/>
</signal>
<signal name="UF_IN">
<contactref element="J1" pad="16"/>
<contactref element="E27" pad="12"/>
</signal>
<signal name="IF0_IN">
<contactref element="J1" pad="15"/>
<contactref element="E27" pad="13"/>
</signal>
<signal name="IF1_IN">
<contactref element="J1" pad="14"/>
<contactref element="E27" pad="4"/>
</signal>
<signal name="IF2_IN">
<contactref element="J1" pad="13"/>
<contactref element="E27" pad="5"/>
</signal>
<signal name="DB_LOAD">
<contactref element="J1" pad="4"/>
<contactref element="E6" pad="12"/>
</signal>
<signal name="N$167">
<contactref element="J1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="E12" pad="10"/>
<contactref element="E24" pad="13"/>
</signal>
<signal name="MD04">
<contactref element="E20" pad="11"/>
<contactref element="E10" pad="14"/>
<contactref element="E14" pad="13"/>
</signal>
<signal name="N$185">
<contactref element="E30" pad="4"/>
<contactref element="E11" pad="8"/>
<contactref element="E12" pad="11"/>
<contactref element="E21" pad="9"/>
</signal>
<signal name="!BCPMA_DISABLE">
<contactref element="E24" pad="2"/>
<contactref element="E12" pad="12"/>
<contactref element="E24" pad="1"/>
</signal>
<signal name="N$218">
<contactref element="E24" pad="12"/>
<contactref element="E3" pad="12"/>
</signal>
<signal name="N$213">
<contactref element="E21" pad="3"/>
<contactref element="E27" pad="9"/>
</signal>
<signal name="N$277">
<contactref element="E2" pad="9"/>
<contactref element="E25" pad="13"/>
</signal>
<signal name="N$308">
<contactref element="E12" pad="2"/>
<contactref element="E18" pad="14"/>
<contactref element="E18" pad="2"/>
</signal>
<signal name="!IOT22_45">
<contactref element="E18" pad="11"/>
<contactref element="E24" pad="10"/>
<contactref element="E24" pad="4"/>
</signal>
<signal name="!IOT21_45">
<contactref element="E18" pad="10"/>
<contactref element="E24" pad="9"/>
<contactref element="E24" pad="5"/>
</signal>
<signal name="!IOT2X5">
<contactref element="E17" pad="14"/>
<contactref element="E12" pad="4"/>
<contactref element="E17" pad="2"/>
</signal>
<signal name="!SKMM">
<contactref element="E17" pad="11"/>
<contactref element="E15" pad="3"/>
</signal>
<signal name="!SKME">
<contactref element="E17" pad="10"/>
<contactref element="E15" pad="5"/>
</signal>
<signal name="!MASKED">
<contactref element="E6" pad="2"/>
<contactref element="E24" pad="6"/>
</signal>
<signal name="N$322">
<contactref element="E6" pad="1"/>
<contactref element="E21" pad="6"/>
</signal>
<signal name="N$338">
<contactref element="E6" pad="6"/>
<contactref element="E9" pad="12"/>
<contactref element="E9" pad="13"/>
</signal>
<signal name="BTP4">
<contactref element="E3" pad="11"/>
<contactref element="E12" pad="8"/>
</signal>
<signal name="BTP3">
<contactref element="E6" pad="11"/>
<contactref element="E15" pad="8"/>
</signal>
<signal name="F_SET">
<contactref element="E6" pad="13"/>
<contactref element="E3" pad="1"/>
<contactref element="E21" pad="13"/>
<contactref element="E25" pad="2"/>
<contactref element="E3" pad="13"/>
<contactref element="E3" pad="4"/>
</signal>
<signal name="CSMME">
<contactref element="E11" pad="6"/>
<contactref element="E3" pad="3"/>
</signal>
<signal name="IOT_FETCH">
<contactref element="E12" pad="5"/>
<contactref element="E21" pad="4"/>
<contactref element="E5" pad="3"/>
</signal>
<signal name="CPMA_DISABLE">
<contactref element="E12" pad="13"/>
<contactref element="E25" pad="3"/>
</signal>
<signal name="N$406">
<contactref element="E15" pad="4"/>
<contactref element="E22" pad="12"/>
<contactref element="E22" pad="11"/>
</signal>
<signal name="SKME">
<contactref element="E15" pad="6"/>
<contactref element="E22" pad="5"/>
</signal>
<signal name="N$409">
<contactref element="E15" pad="12"/>
<contactref element="E19" pad="5"/>
<contactref element="E19" pad="2"/>
<contactref element="E19" pad="3"/>
<contactref element="E19" pad="6"/>
</signal>
<signal name="USETM">
<contactref element="E21" pad="5"/>
<contactref element="E24" pad="8"/>
</signal>
<signal name="N$145">
<contactref element="E33" pad="5"/>
<contactref element="E27" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="R2" pad="1"/>
<contactref element="E34" pad="16"/>
<contactref element="E34" pad="21"/>
<contactref element="E34" pad="9"/>
<contactref element="E34" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="R3" pad="2"/>
<contactref element="E9" pad="6"/>
</signal>
<signal name="!TP3">
<contactref element="E16" pad="3"/>
<contactref element="E15" pad="9"/>
</signal>
<signal name="N$60">
<contactref element="R4" pad="1"/>
<contactref element="C10" pad="+"/>
<contactref element="E11" pad="12"/>
</signal>
<signal name="N$94">
<contactref element="R5" pad="1"/>
<contactref element="C11" pad="+"/>
<contactref element="E11" pad="2"/>
</signal>
<signal name="N$97">
<contactref element="R7" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$91">
<contactref element="R8" pad="2"/>
<contactref element="E22" pad="1"/>
<contactref element="E21" pad="10"/>
</signal>
<signal name="N$32">
<contactref element="J1" pad="2"/>
<contactref element="E21" pad="1"/>
</signal>
<signal name="N$149">
<contactref element="E33" pad="14"/>
<contactref element="E27" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="E20" pad="12"/>
<contactref element="E26" pad="15"/>
</signal>
<signal name="INTERNAL_IO">
<contactref element="R6" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="E16" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="E26" pad="7"/>
<contactref element="E20" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="E26" pad="12"/>
<contactref element="E11" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="E26" pad="14"/>
<contactref element="E20" pad="9"/>
</signal>
<signal name="N$29">
<contactref element="E26" pad="10"/>
<contactref element="E23" pad="9"/>
</signal>
<signal name="N$31">
<contactref element="E26" pad="11"/>
<contactref element="E23" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="R10" pad="2"/>
<contactref element="E26" pad="6"/>
<contactref element="E24" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
