<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>BLANK MODULE W990D</text>
<text>2-69</text>
<text>FLIP CHIP</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="0465">
<description>Drill 0.0465" (#56)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C" library="dec-con" package="0465" value="PAD-0465"/>
<element name="D" library="dec-con" package="0465" value="PAD-0465"/>
<element name="E" library="dec-con" package="0465" value="PAD-0465"/>
<element name="F" library="dec-con" package="0465" value="PAD-0465"/>
<element name="H" library="dec-con" package="0465" value="PAD-0465"/>
<element name="J" library="dec-con" package="0465" value="PAD-0465"/>
<element name="K" library="dec-con" package="0465" value="PAD-0465"/>
<element name="L" library="dec-con" package="0465" value="PAD-0465"/>
<element name="M" library="dec-con" package="0465" value="PAD-0465"/>
<element name="N" library="dec-con" package="0465" value="PAD-0465"/>
<element name="P" library="dec-con" package="0465" value="PAD-0465"/>
<element name="R" library="dec-con" package="0465" value="PAD-0465"/>
<element name="S" library="dec-con" package="0465" value="PAD-0465"/>
<element name="T" library="dec-con" package="0465" value="PAD-0465"/>
<element name="U" library="dec-con" package="0465" value="PAD-0465"/>
<element name="V" library="dec-con" package="0465" value="PAD-0465"/>
<element name="U$2" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="U$4" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="A" library="dec-con" package="0465" value="PAD-0465"/>
<element name="B" library="dec-con" package="0465" value="PAD-0465"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="E" pad="P$1"/>
<contactref element="U$4" pad="E2"/>
</signal>
<signal name="N$2">
<contactref element="H" pad="P$1"/>
<contactref element="U$4" pad="H2"/>
</signal>
<signal name="N$3">
<contactref element="K" pad="P$1"/>
<contactref element="U$4" pad="K2"/>
</signal>
<signal name="N$4">
<contactref element="M" pad="P$1"/>
<contactref element="U$4" pad="M2"/>
</signal>
<signal name="N$5">
<contactref element="P" pad="P$1"/>
<contactref element="U$4" pad="P2"/>
</signal>
<signal name="N$6">
<contactref element="S" pad="P$1"/>
<contactref element="U$4" pad="S2"/>
</signal>
<signal name="N$7">
<contactref element="T" pad="P$1"/>
<contactref element="U$4" pad="T2"/>
</signal>
<signal name="N$9">
<contactref element="D" pad="P$1"/>
<contactref element="U$4" pad="D2"/>
</signal>
<signal name="N$15">
<contactref element="F" pad="P$1"/>
<contactref element="U$4" pad="F2"/>
</signal>
<signal name="N$16">
<contactref element="J" pad="P$1"/>
<contactref element="U$4" pad="J2"/>
</signal>
<signal name="N$17">
<contactref element="L" pad="P$1"/>
<contactref element="U$4" pad="L2"/>
</signal>
<signal name="N$18">
<contactref element="N" pad="P$1"/>
<contactref element="U$4" pad="N2"/>
</signal>
<signal name="N$19">
<contactref element="R" pad="P$1"/>
<contactref element="U$4" pad="R2"/>
</signal>
<signal name="N$20">
<contactref element="U" pad="P$1"/>
<contactref element="U$4" pad="U2"/>
</signal>
<signal name="N$12">
<contactref element="V" pad="P$1"/>
<contactref element="U$4" pad="V2"/>
</signal>
<signal name="N$13">
<contactref element="C" pad="P$1"/>
<contactref element="U$4" pad="C2"/>
</signal>
<signal name="N$8">
<contactref element="B" pad="P$1"/>
<contactref element="U$4" pad="B2"/>
</signal>
<signal name="N$10">
<contactref element="U$4" pad="A2"/>
<contactref element="A" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
