<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="MIL740EXT36">
</package>
</packages>
<symbols>
<symbol name="DS12__">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="A20" direction="in"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="WE" direction="in" function="dot"/>
</symbol>
<symbol name="VCC-GND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DS1270" prefix="IC">
<description>DS1270 and similar NVRAM</description>
<gates>
<gate name="DS1270" symbol="DS12__"/>
<gate name="SUPPLY" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="MIL740EXT36">
<connects>
<connect gate="DS1270" pin="A0" pad="14"/>
<connect gate="DS1270" pin="A1" pad="13"/>
<connect gate="DS1270" pin="A10" pad="25"/>
<connect gate="DS1270" pin="A11" pad="27"/>
<connect gate="DS1270" pin="A12" pad="6"/>
<connect gate="DS1270" pin="A13" pad="30"/>
<connect gate="DS1270" pin="A14" pad="5"/>
<connect gate="DS1270" pin="A15" pad="33"/>
<connect gate="DS1270" pin="A16" pad="4"/>
<connect gate="DS1270" pin="A17" pad="32"/>
<connect gate="DS1270" pin="A18" pad="3"/>
<connect gate="DS1270" pin="A19" pad="35"/>
<connect gate="DS1270" pin="A2" pad="12"/>
<connect gate="DS1270" pin="A20" pad="2"/>
<connect gate="DS1270" pin="A3" pad="11"/>
<connect gate="DS1270" pin="A4" pad="10"/>
<connect gate="DS1270" pin="A5" pad="9"/>
<connect gate="DS1270" pin="A6" pad="8"/>
<connect gate="DS1270" pin="A7" pad="7"/>
<connect gate="DS1270" pin="A8" pad="29"/>
<connect gate="DS1270" pin="A9" pad="28"/>
<connect gate="DS1270" pin="CE" pad="24"/>
<connect gate="DS1270" pin="DQ0" pad="15"/>
<connect gate="DS1270" pin="DQ1" pad="16"/>
<connect gate="DS1270" pin="DQ2" pad="17"/>
<connect gate="DS1270" pin="DQ3" pad="19"/>
<connect gate="DS1270" pin="DQ4" pad="20"/>
<connect gate="DS1270" pin="DQ5" pad="21"/>
<connect gate="DS1270" pin="DQ6" pad="22"/>
<connect gate="DS1270" pin="DQ7" pad="23"/>
<connect gate="DS1270" pin="OE" pad="26"/>
<connect gate="DS1270" pin="WE" pad="31"/>
<connect gate="SUPPLY" pin="GND" pad="18"/>
<connect gate="SUPPLY" pin="VCC" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
