<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="CSX750F">
</package>
<package name="POWERMITE">
<description>&lt;b&gt;Footprint Powermite&lt;/b&gt; SOD80C, SOD87&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/literature/9397/75007774.pdf</description>
</package>
<package name="POWERMITE_LARGEPAD">
<description>&lt;b&gt;Footprint Powermite&lt;/b&gt; SOD80C, SOD87&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/literature/9397/75007774.pdf</description>
</package>
<package name="R-PQFP-N20">
<description>&lt;b&gt;PQFP20&lt;/b&gt; RHL PACKAGE 4.5mm x 3.5mm QFN&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps75003.pdf

Modified to add polarisation marker on tPlace layer</description>
</package>
<package name="RAPC722">
</package>
<package name="RAPC722NT">
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;plastic shrink small outline package; 14 leads; body width 5.3 mm&lt;/b&gt;&lt;p&gt;
SOT337-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
<package name="TO263-7">
</package>
<package name="TO277A_SMPC">
</package>
<package name="TO277A_SMPC_LARGEPAD">
</package>
<package name="TSOP6_VISHAY">
</package>
<package name="TSOP6_VISHAY_LARGEPAD">
</package>
<package name="WE-PD_L/LS/XL/XXL">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_S/M">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_S/M_PLASTIC_BASE">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_XS/XSH_PLASTIC_BASE">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-TPC_2828">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_8015/8012">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_L/LH">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_M/MH">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_S">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_T/TH">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_X">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_XL/XLH">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_XMH">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_XS">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
</packages>
<symbols>
<symbol name="+1V2">
<pin name="+1V2" direction="sup"/>
</symbol>
<symbol name="-L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7407">
<pin name="I" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="7414">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="A4L-LOC">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="JACK-PLUG">
<pin name="BAR" direction="pas"/>
<pin name="PIN" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="LM2679">
<pin name="CB"/>
<pin name="FB" direction="in"/>
<pin name="G@1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IADJ"/>
<pin name="INPUT" direction="in"/>
<pin name="OUTPUT" direction="out"/>
<pin name="SS"/>
</symbol>
<symbol name="P-MOSFET-1G-4D-1S">
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="P-MOSFET-GDS-D">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="QG1">
<pin name="FO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SCHOTTKY_2A">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SN65220">
<pin name="A"/>
<pin name="B"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="TPS75003">
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="FB3" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IS1" direction="in"/>
<pin name="IS2" direction="in"/>
<pin name="OUT3" direction="out"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="SS3" direction="in"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="in"/>
</symbol>
<symbol name="TXB0104">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="GND" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+1V2" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+1V2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A4L-LOC"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CSX750F" prefix="XT">
<gates>
<gate name="G$1" symbol="QG1"/>
</gates>
<devices>
<device name="" package="CSX750F">
<connects>
<connect gate="G$1" pin="FO" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679" prefix="IC">
<description>SIMPLE SWITCHER 5A switch-mode power supply controller&lt;br&gt;

&lt;table&gt;
  &lt;tr&gt;
    &lt;td&gt;Input voltage range:&lt;/td&gt;
    &lt;td&gt;8-40V&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;Output current:&lt;/td&gt;
    &lt;td&gt;5A&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="LM2679"/>
</gates>
<devices>
<device name="" package="TO263-7">
<connects>
<connect gate="G$1" pin="CB" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="G@1" pad="PAD"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IADJ" pad="5"/>
<connect gate="G$1" pin="INPUT" pad="2"/>
<connect gate="G$1" pin="OUTPUT" pad="1"/>
<connect gate="G$1" pin="SS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBRM120LT" prefix="D">
<description>Schottky Diode</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="POWERMITE">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LARGEPAD" package="POWERMITE_LARGEPAD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RAPC722" prefix="J" uservalue="yes">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;br&gt;
Power Jack, DC, Right Angle, Through Hole, Rated 5A at 12VDC, PC Terminals&lt;p&gt;
Distributor: &lt;b&gt;Rapid&lt;/b&gt;&lt;br&gt;
Manufacturer: &lt;b&gt;Switchcraft&lt;/b&gt;&lt;br&gt;
Type: &lt;b&gt;RAPC 722&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="JACK-PLUG"/>
</gates>
<devices>
<device name="" package="RAPC722">
<connects>
<connect gate="G$1" pin="BAR" pad="BARREL"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO_THERMALS" package="RAPC722NT">
<connects>
<connect gate="G$1" pin="BAR" pad="BARREL"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI2323" prefix="Q">
<description>&lt;b&gt;SIPMOS(R) Small-Signal-Transistor&lt;/b&gt; P-Channel, Enhancement mode&lt;p&gt;
Source: http://www.infineon.com/upload/Document/BSP170P_Rev2.4.pdf</description>
<gates>
<gate name="G$1" symbol="P-MOSFET-GDS-D"/>
</gates>
<devices>
<device name="DS-T1-E3" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI3443CDV" prefix="Q">
<gates>
<gate name="G$1" symbol="P-MOSFET-1G-4D-1S"/>
</gates>
<devices>
<device name="" package="TSOP6_VISHAY">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LARGEPAD" package="TSOP6_VISHAY_LARGEPAD">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC07A" prefix="IC">
<description>Hex &lt;b&gt;BUFFER&lt;/b&gt;, open collector high-voltage output</description>
<gates>
<gate name="A" symbol="7407"/>
<gate name="B" symbol="7407"/>
<gate name="C" symbol="7407"/>
<gate name="D" symbol="7407"/>
<gate name="E" symbol="7407"/>
<gate name="F" symbol="7407"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC14A" prefix="IC">
<description>Hex schmitt trigger &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7414"/>
<gate name="B" symbol="7414"/>
<gate name="C" symbol="7414"/>
<gate name="D" symbol="7414"/>
<gate name="E" symbol="7414"/>
<gate name="F" symbol="7414"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DB" package="SSOP14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN65220" prefix="IC">
<description>&lt;b&gt;USB port transient suppressor&lt;/b&gt;&lt;br&gt;
Texas Instruments.</description>
<gates>
<gate name="G$1" symbol="SN65220"/>
</gates>
<devices>
<device name="" package="SOT23-6L">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SS8PH9" prefix="D">
<gates>
<gate name="G$1" symbol="SCHOTTKY_2A"/>
</gates>
<devices>
<device name="" package="TO277A_SMPC">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LARGEPAD" package="TO277A_SMPC_LARGEPAD">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS75003" prefix="IC">
<description>&lt;b&gt;Triple-Supply Power Management IC&lt;/b&gt; for Powering FPGAs and DSPs&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps75003.pdf</description>
<gates>
<gate name="G$1" symbol="TPS75003"/>
</gates>
<devices>
<device name="" package="R-PQFP-N20">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="DGND@1" pad="15"/>
<connect gate="G$1" pin="DGND@2" pad="E@1"/>
<connect gate="G$1" pin="DGND@3" pad="E@2"/>
<connect gate="G$1" pin="DGND@4" pad="E@3"/>
<connect gate="G$1" pin="DGND@5" pad="E@4"/>
<connect gate="G$1" pin="EN1" pad="17"/>
<connect gate="G$1" pin="EN2" pad="4"/>
<connect gate="G$1" pin="EN3" pad="3"/>
<connect gate="G$1" pin="FB1" pad="11"/>
<connect gate="G$1" pin="FB2" pad="10"/>
<connect gate="G$1" pin="FB3" pad="2"/>
<connect gate="G$1" pin="IN1" pad="13"/>
<connect gate="G$1" pin="IN2" pad="8"/>
<connect gate="G$1" pin="IN3" pad="20"/>
<connect gate="G$1" pin="IS1" pad="12"/>
<connect gate="G$1" pin="IS2" pad="9"/>
<connect gate="G$1" pin="OUT3" pad="1"/>
<connect gate="G$1" pin="SS1" pad="16"/>
<connect gate="G$1" pin="SS2" pad="5"/>
<connect gate="G$1" pin="SS3" pad="19"/>
<connect gate="G$1" pin="SW1" pad="14"/>
<connect gate="G$1" pin="SW2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0104" prefix="IC">
<gates>
<gate name="G$1" symbol="TXB0104"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD-Shielded Power Inductors WE-PD&lt;/b&gt;&lt;p&gt;

- Magnetically shielded version which results in a low leakage field&lt;br&gt;
- High storage capacity&lt;br&gt;
- Low self-losses&lt;br&gt;
- Highest possible current loading for SMD-Inducors&lt;br&gt;&lt;br&gt;

-- Switching regulators with low operating voltages
  (computer, laptop, mobile phones, pagers)&lt;br&gt;
-- Integrated DC/DC-converter&lt;br&gt;
-- Is recommended for the application with switching 
regulators from National Semiconductor, Linear Technology,
Texas Instruments and Fairchild Semiconductor, ect.&lt;br&gt;
-- Graphic cards&lt;br&gt;
-- Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications</description>
<gates>
<gate name="G$1" symbol="-L"/>
</gates>
<devices>
<device name="_L/LS/XL/XXL" package="WE-PD_L/LS/XL/XXL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_S/M" package="WE-PD_S/M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_S/M_PLASTIC_BASE" package="WE-PD_S/M_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_XS/XSH_PLASTIC_BASE" package="WE-PD_XS/XSH_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC" prefix="L" uservalue="yes">
<description>&lt;b&gt;Shielded Tiny Power Inductor WE-TPC&lt;/b&gt;&lt;p&gt;

- Extremely flat power inductor&lt;br&gt;
- High current capability&lt;br&gt;
- High reliability and perfect soldering characteristics&lt;br&gt;
  because of integrated soldering pad&lt;br&gt;
- magnetically shielded&lt;br&gt;&lt;br&gt;

-- Portable power like PDA, digital camera,
   PCMICA-cards and displays&lt;br&gt;
-- DC/DC-converter&lt;br&gt;
-- Recommended for switching regulator IC's from
   Linear Technology, National Semiconductor, 
   Texas Instruments and Fairchild Semiconductor</description>
<gates>
<gate name="G$1" symbol="-L"/>
</gates>
<devices>
<device name="_2828" package="WE-TPC_2828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_8015/8012" package="WE-TPC_8015/8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_L/LH" package="WE-TPC_L/LH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_M/MH" package="WE-TPC_M/MH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_S" package="WE-TPC_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_T/TH" package="WE-TPC_T/TH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_X" package="WE-TPC_X">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_XL/XLH" package="WE-TPC_XL/XLH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_XMH" package="WE-TPC_XMH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_XS" package="WE-TPC_XS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
