<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON2">
<description>Single-Height DEC edge connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="ECONOSINGLE">
<description>Economy version of single-height flip chip without gold plated edge connector.</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA18-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="EDGE-CON2" value=""/>
<element name="U$3" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="SV1" library="con-lstb" package="MA18-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="EDGE" library="dec-con" package="ECONOSINGLE" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="SV1" pad="36"/>
<contactref element="U$1" pad="V2"/>
<contactref element="EDGE" pad="V2"/>
</signal>
<signal name="N$2">
<contactref element="SV1" pad="34"/>
<contactref element="U$1" pad="U2"/>
<contactref element="EDGE" pad="U2"/>
</signal>
<signal name="N$3">
<contactref element="SV1" pad="32"/>
<contactref element="U$1" pad="T2"/>
<contactref element="EDGE" pad="T2"/>
</signal>
<signal name="N$4">
<contactref element="SV1" pad="30"/>
<contactref element="U$1" pad="S2"/>
<contactref element="EDGE" pad="S2"/>
</signal>
<signal name="N$5">
<contactref element="SV1" pad="28"/>
<contactref element="U$1" pad="R2"/>
<contactref element="EDGE" pad="R2"/>
</signal>
<signal name="N$6">
<contactref element="SV1" pad="26"/>
<contactref element="U$1" pad="P2"/>
<contactref element="EDGE" pad="P2"/>
</signal>
<signal name="N$7">
<contactref element="SV1" pad="24"/>
<contactref element="U$1" pad="N2"/>
<contactref element="EDGE" pad="N2"/>
</signal>
<signal name="N$8">
<contactref element="SV1" pad="22"/>
<contactref element="U$1" pad="M2"/>
<contactref element="EDGE" pad="M2"/>
</signal>
<signal name="N$9">
<contactref element="SV1" pad="20"/>
<contactref element="U$1" pad="L2"/>
<contactref element="EDGE" pad="L2"/>
</signal>
<signal name="N$10">
<contactref element="SV1" pad="18"/>
<contactref element="U$1" pad="K2"/>
<contactref element="EDGE" pad="K2"/>
</signal>
<signal name="N$11">
<contactref element="SV1" pad="16"/>
<contactref element="U$1" pad="J2"/>
<contactref element="EDGE" pad="J2"/>
</signal>
<signal name="N$12">
<contactref element="SV1" pad="14"/>
<contactref element="U$1" pad="H2"/>
<contactref element="EDGE" pad="H2"/>
</signal>
<signal name="N$13">
<contactref element="SV1" pad="12"/>
<contactref element="U$1" pad="F2"/>
<contactref element="EDGE" pad="F2"/>
</signal>
<signal name="N$14">
<contactref element="SV1" pad="10"/>
<contactref element="U$1" pad="E2"/>
<contactref element="EDGE" pad="E2"/>
</signal>
<signal name="N$15">
<contactref element="SV1" pad="8"/>
<contactref element="U$1" pad="D2"/>
<contactref element="EDGE" pad="D2"/>
</signal>
<signal name="N$16">
<contactref element="SV1" pad="6"/>
<contactref element="U$1" pad="C2"/>
<contactref element="EDGE" pad="C2"/>
</signal>
<signal name="N$17">
<contactref element="SV1" pad="4"/>
<contactref element="U$1" pad="B2"/>
<contactref element="EDGE" pad="B2"/>
</signal>
<signal name="N$18">
<contactref element="SV1" pad="2"/>
<contactref element="U$1" pad="A2"/>
<contactref element="EDGE" pad="A2"/>
</signal>
<signal name="N$19">
<contactref element="SV1" pad="35"/>
<contactref element="U$1" pad="V1"/>
<contactref element="EDGE" pad="V1"/>
</signal>
<signal name="N$20">
<contactref element="SV1" pad="33"/>
<contactref element="U$1" pad="U1"/>
<contactref element="EDGE" pad="U1"/>
</signal>
<signal name="N$21">
<contactref element="SV1" pad="31"/>
<contactref element="U$1" pad="T1"/>
<contactref element="EDGE" pad="T1"/>
</signal>
<signal name="N$22">
<contactref element="SV1" pad="29"/>
<contactref element="U$1" pad="S1"/>
<contactref element="EDGE" pad="S1"/>
</signal>
<signal name="N$23">
<contactref element="SV1" pad="27"/>
<contactref element="U$1" pad="R1"/>
<contactref element="EDGE" pad="R1"/>
</signal>
<signal name="N$24">
<contactref element="SV1" pad="25"/>
<contactref element="U$1" pad="P1"/>
<contactref element="EDGE" pad="P1"/>
</signal>
<signal name="N$25">
<contactref element="SV1" pad="23"/>
<contactref element="U$1" pad="N1"/>
<contactref element="EDGE" pad="N1"/>
</signal>
<signal name="N$26">
<contactref element="SV1" pad="21"/>
<contactref element="U$1" pad="M1"/>
<contactref element="EDGE" pad="M1"/>
</signal>
<signal name="N$27">
<contactref element="SV1" pad="19"/>
<contactref element="U$1" pad="L1"/>
<contactref element="EDGE" pad="L1"/>
</signal>
<signal name="N$28">
<contactref element="SV1" pad="17"/>
<contactref element="U$1" pad="K1"/>
<contactref element="EDGE" pad="K1"/>
</signal>
<signal name="N$29">
<contactref element="SV1" pad="15"/>
<contactref element="U$1" pad="J1"/>
<contactref element="EDGE" pad="J1"/>
</signal>
<signal name="N$30">
<contactref element="SV1" pad="13"/>
<contactref element="U$1" pad="H1"/>
<contactref element="EDGE" pad="H1"/>
</signal>
<signal name="N$31">
<contactref element="SV1" pad="11"/>
<contactref element="U$1" pad="F1"/>
<contactref element="EDGE" pad="F1"/>
</signal>
<signal name="N$32">
<contactref element="SV1" pad="9"/>
<contactref element="U$1" pad="E1"/>
<contactref element="EDGE" pad="E1"/>
</signal>
<signal name="N$33">
<contactref element="SV1" pad="7"/>
<contactref element="U$1" pad="D1"/>
<contactref element="EDGE" pad="D1"/>
</signal>
<signal name="N$34">
<contactref element="SV1" pad="5"/>
<contactref element="U$1" pad="C1"/>
<contactref element="EDGE" pad="C1"/>
</signal>
<signal name="N$35">
<contactref element="SV1" pad="3"/>
<contactref element="U$1" pad="B1"/>
<contactref element="EDGE" pad="B1"/>
</signal>
<signal name="N$36">
<contactref element="SV1" pad="1"/>
<contactref element="U$1" pad="A1"/>
<contactref element="EDGE" pad="A1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
