<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="DIL08">
<description>Dual In Line 8 pin</description>
</package>
<package name="DIL40">
</package>
</packages>
<symbols>
<symbol name="75453">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="PWRGND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SVD-PIC-16C74">
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D8"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="HDIR" direction="in"/>
<pin name="INDEX" direction="out"/>
<pin name="MEMINC" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="in"/>
<pin name="READ" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="TRACK0" direction="out"/>
<pin name="TX" direction="out"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="WRPROT" direction="out"/>
<pin name="_DRIVE0" direction="in"/>
<pin name="_DRIVE1" direction="in"/>
<pin name="_MCLR" direction="in"/>
<pin name="_MEMOE" direction="out"/>
<pin name="_MEMWRT" direction="out"/>
<pin name="_STEP" direction="in"/>
<pin name="_WGATE" direction="in"/>
<pin name="_WRITE" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="75453" prefix="IC">
<description>Dual NAND peripheral driver</description>
<gates>
<gate name="A" symbol="75453"/>
<gate name="B" symbol="75453"/>
<gate name="P" symbol="PWRGND"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="7"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SVD-PIC16C74" uservalue="yes">
<gates>
<gate name="G$1" symbol="SVD-PIC-16C74"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A10" pad="35"/>
<connect gate="G$1" pin="A11" pad="36"/>
<connect gate="G$1" pin="A12" pad="37"/>
<connect gate="G$1" pin="A13" pad="38"/>
<connect gate="G$1" pin="A14" pad="39"/>
<connect gate="G$1" pin="A15" pad="40"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="3"/>
<connect gate="G$1" pin="A8" pad="33"/>
<connect gate="G$1" pin="A9" pad="34"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="20"/>
<connect gate="G$1" pin="D2" pad="21"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="27"/>
<connect gate="G$1" pin="D5" pad="28"/>
<connect gate="G$1" pin="D6" pad="29"/>
<connect gate="G$1" pin="D8" pad="30"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="31"/>
<connect gate="G$1" pin="HDIR" pad="5"/>
<connect gate="G$1" pin="INDEX" pad="16"/>
<connect gate="G$1" pin="MEMINC" pad="8"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="READ" pad="15"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="TRACK0" pad="23"/>
<connect gate="G$1" pin="TX" pad="25"/>
<connect gate="G$1" pin="VCC@1" pad="11"/>
<connect gate="G$1" pin="VCC@2" pad="32"/>
<connect gate="G$1" pin="WRPROT" pad="24"/>
<connect gate="G$1" pin="_DRIVE0" pad="17"/>
<connect gate="G$1" pin="_DRIVE1" pad="18"/>
<connect gate="G$1" pin="_MCLR" pad="1"/>
<connect gate="G$1" pin="_MEMOE" pad="9"/>
<connect gate="G$1" pin="_MEMWRT" pad="10"/>
<connect gate="G$1" pin="_STEP" pad="6"/>
<connect gate="G$1" pin="_WGATE" pad="4"/>
<connect gate="G$1" pin="_WRITE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
