<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="SO16">
<description>SOIC 16 3.9mm</description>
</package>
</packages>
<symbols>
<symbol name="DS1321">
<pin name="BW#" direction="out"/>
<pin name="CEI1#" direction="in"/>
<pin name="CEI2#" direction="in"/>
<pin name="CEI3#" direction="in"/>
<pin name="CEI4#" direction="in"/>
<pin name="CEO1#" direction="out"/>
<pin name="CEO2#" direction="out"/>
<pin name="CEO3#" direction="out"/>
<pin name="CEO4#" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="MODE" direction="pas"/>
<pin name="RST#" direction="out"/>
<pin name="TOL" direction="in"/>
<pin name="VBAT" direction="in"/>
<pin name="VCCI" direction="in"/>
<pin name="VCCO" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DS1321" prefix="IC">
<description>DS1321 Battery Monitor</description>
<gates>
<gate name="G$1" symbol="DS1321"/>
</gates>
<devices>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="BW#" pad="14"/>
<connect gate="G$1" pin="CEI1#" pad="4"/>
<connect gate="G$1" pin="CEI2#" pad="5"/>
<connect gate="G$1" pin="CEI3#" pad="6"/>
<connect gate="G$1" pin="CEI4#" pad="7"/>
<connect gate="G$1" pin="CEO1#" pad="13"/>
<connect gate="G$1" pin="CEO2#" pad="12"/>
<connect gate="G$1" pin="CEO3#" pad="11"/>
<connect gate="G$1" pin="CEO4#" pad="10"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="MODE" pad="9"/>
<connect gate="G$1" pin="RST#" pad="15"/>
<connect gate="G$1" pin="TOL" pad="3"/>
<connect gate="G$1" pin="VBAT" pad="2"/>
<connect gate="G$1" pin="VCCI" pad="16"/>
<connect gate="G$1" pin="VCCO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
