{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"flags":["formulas_cached_only"]}
["Qty","Value","Device","Package","Mouser","Description","Parts"]
[6,".22uF","C-US050-025X075","C050-025X075",null,"CAPACITOR, American symbol","C2, C3, C4, C5, C6, C7"]
[1,"47uF","CPOL-USE5-8.5","E5-8,5",null,"POLARIZED CAPACITOR, American symbol","C1"]
[2,"GREEN","LED5MM","LED5MM",null,"LED","GREEN, PWR"]
[2,"YELLOW","LED5MM","LED5MM",null,"LED","YELLOW, UUT_PWR"]
[2,"RED","LED5MM","LED5MM",null,"LED","RED1, RED2"]
[1,null,"MA13-2","MA13-2",null,"PIN HEADER","PC1"]
[1,null,"MTA06-156","1X6MTA",null,"AMP connector","POWER"]
[19,null,"PINHD-1X1","1X01",null,"PIN HEADER","19 Single Pin Headers"]
[1,"100K","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R1"]
[2,"180 ohm","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R6, R7"]
[2,"1K","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R12, R13"]
[2,"1N4001","1N4004","DO41-10",null,"DIODE","D1, D2"]
[1,"2K","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R10"]
[5,"300 ohm","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R2, R3, R4, R5, R14"]
[1,"5.6K","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R11"]
[2,"560 ohm","R-US_0207/10","0207/10",null,"RESISTOR, American symbol","R8, R9"]
[1,"710x","710x","7109MD9V3",null,"710x with optional V2 or V3 mounting bracket.","UUT"]
[1,"74LS06N","74LS06N","DIL14",null,"Hex INVERTER, open collector high-voltage output","IC6"]
[1,"Ax1","PINHD-2X18","2X18",null,"PIN HEADER","AX1"]
[1,"Ax2","PINHD-2X18","2X18",null,"PIN HEADER","AX2"]
[1,"Bx1","PINHD-2X18","2X18",null,"PIN HEADER","BX1"]
[1,"Bx2","PINHD-2X18","2X18",null,"PIN HEADER","BX2"]
[2,"M916","M916","H807","x","Simple 36 pin connector/wire cable","A, B"]
[5,"MCP23S17SP","MCP23S17SP","DIL28-3",null,"16-Bit I/O Expander with Serial Interface","IC1, IC2, IC3, IC4, IC5"]
[]
[]
["Assembly instructions at http://www.so-much-stuff.com/pdp8/repair/fc-tester/assembly.php"]

{"sheet":"Sheet2","index":1,"n_rows":14,"n_cols":4,"rows_kept":14,"flags":["formulas_cached_only"]}
["Who","Kit","PCB"]
["Malcolm",1,1]
["Michael Thompson",2,null,"Done"]
["Jack",2,null,"Done"]
["UMD",2]
["Kyle",1,null,"Done"]
["Doug",1,null,"RasPi"]
["Bob Rosenbloom",1,null,"RasPi"]
["Bill Maddox",1,null,"RasPi"]
["Pavl Zachary",1,null,"Wants RasPi"]
["James Markevitch",1,null,"Wants RasPi"]
[]
[]
["Total",13,1]

{"sheet":"Sheet3","index":2,"n_rows":12,"n_cols":2,"rows_kept":12,"flags":["formulas_cached_only"]}
[]
["PCB",{"v":97.62,"d":"$97.62"}]
["Mouser",{"v":433.5,"d":"$433.50"}]
["Shunt 1",{"v":55.84,"d":"$55.84"}]
["Shunt 2",{"v":32.1,"d":"$32.10"}]
["Power C.",{"v":20,"d":"$20.00"}]
["EDAC",{"v":346.8,"d":"$346.80"}]
[]
["Total",{"v":985.8600000000001,"d":"$985.86"}]
["Each",{"v":49.293000000000006,"d":"$49.29"}]
["Shipping",{"v":10.48,"d":"$10.48"}]
["Sum",{"v":59.77300000000001,"d":"$59.77"}]