<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>Install socket E1 on solder side.</text>
</plain>
<libraries>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E1" library="ic-package" package="DIL16" value=""/>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="U$2" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="E1" pad="8"/>
<contactref element="U$2" pad="J2"/>
</signal>
<signal name="N$2">
<contactref element="E1" pad="1"/>
<contactref element="U$2" pad="A2"/>
</signal>
<signal name="N$3">
<contactref element="E1" pad="13"/>
<contactref element="U$2" pad="P2"/>
</signal>
<signal name="N$4">
<contactref element="E1" pad="7"/>
<contactref element="U$2" pad="H2"/>
</signal>
<signal name="N$5">
<contactref element="E1" pad="6"/>
<contactref element="U$2" pad="F2"/>
</signal>
<signal name="N$6">
<contactref element="E1" pad="5"/>
<contactref element="U$2" pad="E2"/>
</signal>
<signal name="N$7">
<contactref element="E1" pad="4"/>
<contactref element="U$2" pad="D2"/>
</signal>
<signal name="N$8">
<contactref element="E1" pad="3"/>
<contactref element="U$2" pad="C2"/>
</signal>
<signal name="N$9">
<contactref element="E1" pad="2"/>
<contactref element="U$2" pad="B2"/>
</signal>
<signal name="N$10">
<contactref element="E1" pad="16"/>
<contactref element="U$2" pad="T2"/>
</signal>
<signal name="N$11">
<contactref element="E1" pad="15"/>
<contactref element="U$2" pad="S2"/>
</signal>
<signal name="N$12">
<contactref element="E1" pad="14"/>
<contactref element="U$2" pad="R2"/>
</signal>
<signal name="N$13">
<contactref element="E1" pad="9"/>
<contactref element="U$2" pad="K2"/>
</signal>
<signal name="N$14">
<contactref element="E1" pad="10"/>
<contactref element="U$2" pad="L2"/>
</signal>
<signal name="N$15">
<contactref element="E1" pad="11"/>
<contactref element="U$2" pad="M2"/>
</signal>
<signal name="N$16">
<contactref element="E1" pad="12"/>
<contactref element="U$2" pad="N2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
