<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="-0.0001" y2="0" width="0" layer="20"/>
<wire x1="-0.0001" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="27.9401" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="80.9624" width="0" layer="20"/>
<wire x1="0" y1="80.9624" x2="27.9401" y2="80.9624" width="0" layer="20"/>
<wire x1="27.9401" y1="0" x2="27.9401" y2="80.9624" width="0" layer="20"/>
<text>Regulator Board</text>
<text>VRS</text>
</plain>
<libraries>
<library name="holes">
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="0635">
<description>Drill 0.0635" (#52)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$5" library="holes" package="3,6" value=""/>
<element name="U$6" library="holes" package="3,6" value=""/>
<element name="U$7" library="holes" package="3,6" value=""/>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="RING2" library="dec-con" package="0635" value="PAD-0635"/>
<element name="RING" library="dec-con" package="0635" value="PAD-0635">
<attribute name="NAME"/>
</element>
<element name="TIP" library="dec-con" package="0635" value="PAD-0635">
<attribute name="NAME"/>
</element>
<element name="+15V" library="dec-con" package="0635" value="PAD-0635">
<attribute name="NAME"/>
</element>
<element name="GND" library="dec-con" package="0635" value="PAD-0635"/>
<element name="TIPSW" library="dec-con" package="0635" value="PAD-0635"/>
<element name="+15VIN" library="dec-con" package="0635" value="PAD-0635"/>
<element name="+5V" library="dec-con" package="0635" value="PAD-0635">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="+15V">
<contactref element="+15V" pad="P$1"/>
<contactref element="+15VIN" pad="P$1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="RING" pad="P$1"/>
<contactref element="RING2" pad="P$1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="TIP" pad="P$1"/>
<contactref element="TIPSW" pad="P$1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="3"/>
<contactref element="+5V" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
