<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>Secure Digital card connector Kingfont SDCMF-109XXW0X0

SDCMF-109aaW0b0
aa:
05 = 5u" gold plating
10 = 10u" gold plating
15 = 15u" gold plating

b:
1 = tin-lead 90/10
T = lead free</description>
<packages>
<package name="SDCMF-10915W010">
<description>SD card connector
KINGFONT SDCMF-10915W010</description>
</package>
<package name="SDBMF-00915B0T2">
<description>SDBMF-00915B0T2 (Farnell, Newark)</description>
</package>
<package name="SCDA1A">
<description>SCDA1A0900, SCDA1A0901, SCDA1A0801, SCDA1A1301, SCDA1A1401, SCDA1A1501
(Mouser)</description>
</package>
<package name="WM24032">
<description>500998-0900 (Digikey)</description>
</package>
<package name="SCDA5A">
</package>
</packages>
<symbols>
<symbol name="SDCARD_SYMBOL">
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD/DI"/>
<pin name="CLK/SCLK"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="WP" direction="out"/>
<pin name="CDI#" direction="out"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
</symbol>
<symbol name="SCDARD">
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD/DI"/>
<pin name="CLK/SCLK"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="WP" direction="out"/>
<pin name="CD#" direction="out"/>
<pin name="CMN" direction="in"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SDCARD_OLD" uservalue="yes">
<description>SD card connector
KINGFONT SDCMF-10915W010</description>
<gates>
<gate name="G$1" symbol="SDCARD_SYMBOL"/>
</gates>
<devices>
<device name="VAR1" package="SDCMF-10915W010">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CDI#" pad="11"/>
<connect gate="G$1" pin="CLK/SCLK" pad="5"/>
<connect gate="G$1" pin="CMD/DI" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="13"/>
<connect gate="G$1" pin="GND3" pad="14"/>
<connect gate="G$1" pin="GND4" pad="15"/>
<connect gate="G$1" pin="GND5" pad="16"/>
<connect gate="G$1" pin="GND6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDCARD" prefix="J">
<description>SD Card Holder</description>
<gates>
<gate name="G$1" symbol="SCDARD"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="GND"/>
</gates>
<devices>
<device name="DIGIKEY" package="WM24032">
<connects>
<connect gate="G$1" pin="CD#" pad="CD"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK/SCLK" pad="5"/>
<connect gate="G$1" pin="CMD/DI" pad="2"/>
<connect gate="G$1" pin="CMN" pad="CMN"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@2" pad="6"/>
<connect gate="G$1" pin="WP" pad="WP"/>
<connect gate="G$2" pin="GND" pad="A1"/>
<connect gate="G$3" pin="GND" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEWARK" package="SDBMF-00915B0T2">
<connects>
<connect gate="G$1" pin="CD#" pad="SW1"/>
<connect gate="G$1" pin="CD/DAT3" pad="DAT3"/>
<connect gate="G$1" pin="CLK/SCLK" pad="CLK"/>
<connect gate="G$1" pin="CMD/DI" pad="CMD"/>
<connect gate="G$1" pin="CMN" pad="SW3"/>
<connect gate="G$1" pin="DAT0" pad="DAT0"/>
<connect gate="G$1" pin="DAT1" pad="DAT1"/>
<connect gate="G$1" pin="DAT2" pad="DAT2"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VSS@1" pad="VSS$1"/>
<connect gate="G$1" pin="VSS@2" pad="VSS$2"/>
<connect gate="G$1" pin="WP" pad="SW2"/>
<connect gate="G$2" pin="GND" pad="GND$1"/>
<connect gate="G$3" pin="GND" pad="GND$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOUSER" package="SCDA1A">
<connects>
<connect gate="G$1" pin="CD#" pad="10"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK/SCLK" pad="5"/>
<connect gate="G$1" pin="CMD/DI" pad="2"/>
<connect gate="G$1" pin="CMN" pad="11"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@2" pad="6"/>
<connect gate="G$1" pin="WP" pad="12"/>
<connect gate="G$2" pin="GND" pad="13"/>
<connect gate="G$3" pin="GND" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UNKNOWN" package="SDCMF-10915W010">
<connects>
<connect gate="G$1" pin="CD#" pad="11"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK/SCLK" pad="5"/>
<connect gate="G$1" pin="CMD/DI" pad="2"/>
<connect gate="G$1" pin="CMN" pad="15"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@2" pad="6"/>
<connect gate="G$1" pin="WP" pad="10"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$3" pin="GND" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SCDA5A">
<connects>
<connect gate="G$1" pin="CD#" pad="10"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK/SCLK" pad="5"/>
<connect gate="G$1" pin="CMD/DI" pad="2"/>
<connect gate="G$1" pin="CMN" pad="11"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@2" pad="6"/>
<connect gate="G$1" pin="WP" pad="12"/>
<connect gate="G$2" pin="GND" pad="13"/>
<connect gate="G$3" pin="GND" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
